{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["招标清单","议标清单","远程议标清单"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"招标清单","index":0,"n_rows":767,"n_cols":4,"rows_kept":767,"flags":["formulas_cached_only"]}
["物料编码","物料名称","规格","合计数量"]
["J150201130","PC膜","阻燃PC 平米",30000]
["Y320601363","线路板","双层板 带碳油 平米",50000]
["Y320601364","线路板","双层板 不带碳油 平米",10000]
["Y210300036","液晶屏","II-H47194F9.5-3.0V",700000]
["Y210100363","液晶屏","CGG128024C00-FGN-R-01-A(A)",60000]
["Y210100345","液晶屏","II-66403T11-3.0V ",195000]
["Y210100344","液晶屏","II-66413T11-3.0V ",50000]
["Y210100341","液晶屏","II-66406T25-3.0V ",175000]
["Y210100335","液晶屏","II-6028T24.6-3.0V ",240000]
["Y210100333","液晶屏","II-66405T15-3.0V ",50000]
["Y210100325","液晶屏","II-66407T15-3.0V ",6000]
["Y210100324","液晶屏","II-66400T15-3.0V ",620000]
["Y210100322","液晶屏","II-66403T09-3.0V ",144000]
["Y210100301","液晶屏","II-66310T11.7-3.0V ",100000]
["Y210100300","液晶屏","II-CGS145B01T11-3.1V",320000]
["Y210100281","液晶屏","CGG208080A02-FHN-R 插 ",40000]
["Y210100278","液晶屏","II-21D03C6T27-W-3.0VH(HTN高耐久)  ",250000]
["Y210100273","液晶屏","II-D1708067T09-3.0V ",425000]
["Y210100272","液晶屏","II-21D03C6T27-W-3.0VX(FSTN高耐久) 插 ",300000]
["Y210100271","液晶屏","21S03C8T28-W-5.0V（FSTN 高耐久）插 ",200000]
["Y210100268","液晶屏","II-66216F15-3.0V",425000]
["Y210100265","液晶屏","20H03C8T28-W-5.0VX(高耐久) ",510000]
["Y210100264","液晶屏","3061WT25-3.1VX(高耐久) ",1200000]
["Y210100263","液晶屏","II-D1708066T09-3.0V",378000]
["Y210100241","液晶屏","II-66300F12.7-3.0V",10000]
["Y210100237","液晶屏","II-66213F15-3.0V ",62000]
["Y200100178","背光板","ARD-6725W1A0-21-NG-A ",60000]
["Y200100169","背光板","ARD-5825W1A0-5.3-NG",144000]
["Y200100167","背光板","GC01W6927QS-Y34.6A-NG ",40000]
["Y200100158","背光板","ARD-5924W1A0-21-NG ",240000]
["Y200100152","背光板","ARD-6626W1A0-21.2-NG ",175000]
["Y200100151","背光板","ARD-5725W1A0-11.6-NG ",50000]
["Y200100150","背光板","ARD-5725W1A0-8-NG",195000]
["Y200100149","背光板","ARD-5725W1A0-5.3-NG-A",803000]
["Y200100147","背光板","GC01W10054LG-Y23.4-A ",480000]
["Y200100145","背光板","GC01W10054LG-Y23.4 ",30000]
["Y200100144","背光板","ARD-6223B1A0-7.4-NG ",100000]
["Y200100143","背光板","CGS145B00-HHW-R",370000]
["Y200100132","背光板","C01W7131NG-P11.6 ",1107000]
["Y200100128","背光板","GC01W7231NG-Y23.5-NW21",550000]
["Y200100119","背光板","GC01W7231NG-Y22-GW20",1200000]
["Y200100117","背光板","T02W9954NG-Y23.4-P2 ",200000]
["Y200100102","背光板","C01W6218NG-P9A（）",10000]
["Y190400100","SIM卡","电信nbiot工业级(正式 6年资费)",500000]
["Y190400010","射频卡","T5557(水表)",300000]
["Y190300161","用户卡","PVC,哑光，85.5×54mm，t=0.76±0.2mm，图号：LGG8.865.006-NP43",20000]
["Y190300159","用户卡","PVC,哑光，85.5×54mm，t=0.76±0.2mm，图号：LGG8.865.006-NP41",25000]
["Y190300156","用户卡","PVC,哑光，85.5×54mm，t=0.76±0.2mm，图号：LGG8.865.006-NP38",20000]
["Y190300153","用户卡","PVC,哑光，85.5×54mm，t=0.76±0.2mm，图号：LGG8.865.006-NP35",250000]
["Y190300152","用户卡","PVC,哑光，85.5×54mm，t=0.76±0.2mm，图号：LGG8.865.006-NP34",100000]
["Y190300151","用户卡","PVC,哑光，85.5×54mm，t=0.76±0.2mm，图号：LGG8.865.006-NP33",400000]
["Y190300148","用户卡","PVC,哑光，85.5×54mm，t=0.76±0.2mm，图号：LGG8.865.006-NP30",12000]
["Y180400061","干电池","7号 LR03 1.5V",400000]
["Y170100004","卡座","SIM卡座 贴",600000]
["Y160100068","光耦","R-440AS-TP 贴 ",300000]
["Y160100057","光耦","ORPC-817SC-H-D2S-TP-C-V ",200010]
["Y160100028","光耦","LTV816STP-D3-TXCU",6550000]
["Y160100010","光耦","EL816S1(D) 贴",25350000]
["Y150100009","桥堆","MB6S",1750000]
["Y130100010","蜂鸣器","TMB12A03(3.3V) ROHS 无铅",300000]
["Y130100009","蜂鸣器","YX-WY1255 (φ12)(压电无源)",170000]
["Y130100002","蜂鸣器","TMB12A03(3.3V)",2815005]
["Y120100109","晶体座","iH2603B 贴",80000]
["Y120200096","晶振","SMD3225-4P-25MHz 负载电容8pF 调整频差±10ppm 温度频差 ±30ppm 贴 无源",40000]
["Y120200090","晶振","49SMD-3.579545MHz-3P（三脚）(调频±20PPM温频±20PPM C=20PF)贴 ",40000]
["Y120200061","晶振","32.768kHz（SSP-T7-F）日本精工",3746000]
["Y120100108","晶振","VT-200-F型32.768kHz精工 插(格州定制)2",80000]
["Y120100088","晶振","49S-3.579545MHz 插 (通用) L=3.5",1750000]
["Y120100084","晶振","32.768KHz 12.5pF ±20ppm(SP-T2A-F贴）",670000]
["Y120100077","晶振","49SMD-5.5296MHz-3P（三脚）负载电容15pF  调整频差10ppm 温度频差15ppm 贴",459000]
["Y120100053","晶振","49SMD-8.192MHz-3P 负载电容15pF 调整频差20ppm 温度频差30ppm 贴",400000]
["Y120100019","晶振","VT-200-F型32.768kHz精工 插(格州定制)1",2250000]
["Y120100015","晶振","VT-200-F型32.768kHz精工 插",210000]
["Y110500008","耦合变压器","FH9111",400000]
["Y110500005","载波耦合线圈","T6-YY156100（100μH 1:1 耦合变压器）",20605]
["Y110300007","场效应管","L2N7002LT1G SOT-23 贴",50000]
["Y110300003","场效应管","2N7002 贴",200020]
["Y110100027","共模滤波器","JK-UU9802T ",173000]
["Y110100026","共模滤波器","EE8.3-20mH",440000]
["Y110100020","共模滤波器","UU9.8-KD-33mH ",951000]
["Y101100647","集成电路","SGM2212-3.3XOB2G/TR(T0-252-2)贴 ",20000]
["Y101100626","集成电路","SGM66099C-ADJYTDI6G/TR，封装TDFN-2*2-6AL，() 贴",170000]
["Y101100593","集成电路","GD25Q64ESIGR 贴(GD)",430000]
["Y101100582","集成电路","LESDA6V1W5T1G 贴",175000]
["Y101100565","集成电路","SCM402FB(14*14) 贴 ",40000]
["Y101100557","集成电路","GD25Q16ESIG3 SOP8 贴",745000]
["Y101100556","集成电路","GD25Q32ESIG3 SOP8 贴",302050]
["Y101100540","集成电路","GD25Q32ESIGR 贴 ",1200000]
["Y101100538","集成电路","GD25Q256EYIG3 WSON8(8mm*6mm) 贴 ",80000]
["Y101100530","集成电路","SGM61410XN6G/TR",260000]
["Y101100493","集成电路","TK8021 SOT23-6 贴",500000]
["Y101100477","集成电路","LA1631 SOT23-6 ",710000]
["Y101100454","集成电路","SGM2034-3.3YN3G/TR SOT23 贴 ",695000]
["Y101100443","集成电路","SGM61411XN6G/TR 贴",945000]
["Y101100419","集成电路","SGM8708YN8G/TR SOT-23-8 贴 ",40000]
["Y101100417","集成电路","SGM48755YMS10G/TR 贴 ",40000]
["Y101100416","集成电路","SGM7SZ126YN5G/TR(SOT-23-5封装)贴 ",160000]
["Y101100408","集成电路","GD25Q64ESIGR 贴",500000]
["Y101100401","集成电路","SGM61230XTN6G/TR 贴",600000]
["Y101100397","集成电路","SGM2203-5.75YK3G/TR ",1595000]
["Y101100396","集成电路","SGM2203-3.6YK3G/TR 贴",453000]
["Y101100388","集成电路","SGM2203-4.0YK3G 贴",150000]
["Y101100383","集成电路","SGM2205-12XK3G/TR SOT-89 贴 ",670000]
["Y101100377","集成电路","SGM2203-3.3YK3G/TR 贴",1423625]
["Y101100376","集成电路","SGM6623  贴",1087445]
["Y101100357","集成电路","SGM2523A 贴 ",2029000]
["Y101100297","集成电路","SGM2040-3.3YN5G/TR SOT-23-5 贴 ",150000]
["Y101100279","集成电路","WS4680QE-6/TR(可替代AL868) 贴",3898000]
["Y101100241","集成电路","SGM2203-3.3YN3LG/TR 贴",1888000]
["Y101100227","集成电路","SGM2203-5.0YK3G/TR 贴 ",5974010]
["Y101100178","集成电路","SGC6101C 贴 ",410000]
["Y101100165","集成电路","DRV8837 贴",700000]
["Y101100129","集成电路","M24512-RMN6TP 贴",748000]
["Y101100128","集成电路","M24256-BRMN6TP 贴",620000]
["Y101100036","集成电路","NSQA6V8AW5T2G 贴",425000]
["Y100900020","集成电路","PY25Q16HB-SUG-IR 贴 ",770000]
["Y100700198","集成电路","M24512E-FMN6TP 贴",305000]
["Y100700182","集成电路","MD5230 SOT-23 贴",600000]
["Y100700181","集成电路","MD85E57PA1 SOT-89 贴   ",480000]
["Y100700173","集成电路","M24256E-FMN6TP 贴",2524720]
["Y100700172","集成电路","MD5130 SOT-23 贴 ",510000]
["Y100700169","集成电路","MX25V1606FM2I03 贴",112010]
["Y100700161","集成电路","MD8333 SO-T89 贴 ",400000]
["Y100700158","集成电路","MX25L6433FM2I 贴",330000]
["Y100700155","集成电路","MD85E50PA1 SOT89-3L贴 ",80000]
["Y100700154","集成电路","MD8340 SOT89 贴 ",89000]
["Y100700120","集成电路","MD5330 SOT-23 贴 ",200000]
["Y100700116","集成电路","MX25L1606E 贴",120000]
["Y100700079","集成电路","MD5336 SOT-23 贴 ",710000]
["Y100700078","集成电路","MD5333 SOT-23 贴 ",1710000]
["Y100700060","集成电路","MP2451DT-LF-Z 贴",550000]
["Y100700059","集成电路","MT1322AT SOT-23 贴",2383060]
["Y100300019","集成电路","CYT431A SOT23 贴",2998445]
["Y100200074","集成电路","BL3090 贴 ",60000]
["Y100200073","集成电路","BL24C512A-PARC SOP-8 贴 ",770000]
["Y100200069","集成电路","BL13232ESO 贴 ",300000]
["Y100200068","集成电路","BL5616 SOP8 贴 ",40000]
["Y100200065","集成电路","BL9342(车规) SOT23-6L 贴 ",1200000]
["Y100200060","集成电路","BL55088 LQFP52 贴 ",25000]
["Y100200050","集成电路","BL24C256A ",310000]
["Y100200049","集成电路","BL3085（有极性） 贴",2049460]
["Y100200048","集成电路","BL3085N(无极性) ",90000]
["Y100200047","集成电路","BL55080 贴 ",310000]
["Y100200072","RS485芯片","BL3085(I47)-T（有极性） 贴",1600000]
["Y090500108","红外发射接收管","L3IR4-45D-ED-W(2.2)(11.5)、2CU302IR-LM/D-W(2.2)(11.5)（灯加灯座组装成品） ",20000]
["Y090500107","远红外接收管","IRM6538S-5-O 插  L=3.5±0.5mm ",10000]
["Y090500104","红外光敏管","AT405-PD-01 (万州）L=3.5mm",1739000]
["Y090500096","红外发射接收管","L5IR4-45D1-FD-TK/W0038K5-30-W2(26.5)-D1-72H L=22.5mm/26.5mm (新晶圆)低功耗",430000]
["Y090500093","红外发射接收管","L5IR4-45D1-FD-TK/W0038K5-30-W2(24.5)-D1-72H L=21/24.5mm (新晶圆)",250000]
["Y090500087","红外发射管","AT205 L=3.5mm",1749000]
["Y090500073","红外发射接收管","L5IR4-45D1-FD-TK/W0038K5-30-W2(4.5)-D1-72H nbspL=3.5mm/4.5mm  ",500000]
["Y090500063","红外发射接收管","L3IR4-45D-ED-W(2.2)(11.5)、2CU302IR-LM/D-W(2.2)(11.5)",120000]
["Y090500042","红外发射管","AT205",320000]
["Y090500040","红外发射接收管","AT205/HM338RL-W 可得 原脚长",1780000]
["Y090500007","红外光敏管","AT405-PD-01",320000]
["Y090400092","发光二极管","0805 侧贴 黄色",475000]
["Y090400091","发光二极管","0805 侧贴 绿色",495000]
["Y090400090","发光二极管","0805 侧贴 红色",1030000]
["Y090400084","发光二极管","WZW1206-DTZ 贴",980000]
["Y090400083","发光二极管","WZYG1205-TR8-DTZ 绿 贴",1447000]
["Y090400080","发光二极管","0805 绿",1002000]
["Y090400076","发光二极管","0805 黄",1131000]
["Y090400075","发光二极管","0805 红",4099000]
["Y090400066","发光二极管","WZY1205-TR8-DTZ 黄 贴 ",1200000]
["Y090400065","发光二极管","WZR1205-TR8-DTZ 红 贴 ",6271000]
["Y090400063","发光二极管","WZW1205-TR8-DTZ 贴",3788000]
["Y090400055","发光二极管","23-21B/Y2C-AQ1R2/2A-2V-15MCD20mA-LED1205-FAN 黄 贴",850000]
["Y090400032","发光二极管","23-21BSURC/S530-A2/TR8(DYDX)-2V-15MCD20mA-LED1205-FAN 红 贴",5030000]
["Y090400031","发光二极管","23-21BSYGC/S530-E3/TR8(DYDX)-2V-22MCD20mA-LED1205-FAN 绿 贴",1195000]
["Y090300137","三极管","S9013(120-200档) 端子测温专用 贴 ",160000]
["Y090300063","三极管","LMBT5551LT1G 贴 ",272025]
["Y090300012","三极管","S8550D 贴",23570445]
["Y090300011","三极管","S8050D 贴",36197020]
["Y090200364","TSS管","SPE06RBLD ",1200000]
["Y090200363","TSS管","LTPA065A SMA ",370000]
["Y090200329","MOS管","SP3407S 贴 ",300000]
["Y090300086","MOS管","LN2302LT1G 贴",240000]
["Y090200124","MOS管","LP2301LT1G 贴 ",7041010]
["Y090200287","TVS管","ESD5451N-2/TR 贴 ",800000]
["Y090200281","TVS管","LTVB6.0CJ（SMBJ6.0CA）贴 ",550000]
["Y090200224","TVS管","WS4.5DPV（单向）",175000]
["Y090200146","TVS管","SMBJ180A 贴",26000]
["Y090200142","TVS管","SMBJ36CA 贴",740000]
["Y090200198","TVS管","SMBJ15A 贴 ",1907000]
["Y090200103","TVS管","WP61065A  贴",580000]
["Y090200036","TVS管","SMBJ6.0CA 贴",2031885]
["Y090200386","TVS管","SMF36A SOD123FL",600000]
["Y090200384","TVS管","LTVL36AD  SOD-123FL 贴 ",1290000]
["Y090200379","TVS管","SMBJ15A 贴  ",400000]
["Y101100018","二极管","LBAT54CLT1G 贴",8387000]
["Y090200304","二极管","1N4007 贴",3100000]
["Y090200298","二极管","DFR1M(F1M） SOD-123FL 贴 ",80000]
["Y090200365","二极管","SM160W  SOD123FL 贴 ",160000]
["Y090200435","二极管","ES2J SMA 贴 ",50000]
["Y090200431","二极管","EM540A 贴 ",200000]
["Y090200421","二极管","LT4007L 贴 ",3345000]
["Y090200420","二极管","EM540AG(SMA-W) 贴 ",480000]
["Y090200223","二极管","BAV23CLT1G 贴 ",5000000]
["Y090200203","二极管","B340A 贴",175000]
["Y090200201","二极管","ES1M SMA 贴",640000]
["Y090200196","二极管","EM520AG ",7704000]
["Y090200176","二极管","M20 贴",10541000]
["Y090200175","二极管","ES3G SMB 贴",1660000]
["Y090200139","二极管","BZX84C4V7LT1 贴",1200000]
["Y090200129","二极管","LMBD7000LT1G贴 ",310000]
["Y090200128","二极管","LBAT54ALT1G 贴 ",75000]
["Y090200127","二极管","RS1G 贴 ",776000]
["Y090200126","二极管","LBAT54HT1G 贴 ",7618000]
["Y090200125","二极管","1N4148WS 贴 ",490050]
["Y090200110","二极管","SS16 贴1",279025]
["Y090200109","二极管","SS16 贴",3800435]
["Y090200106","二极管","US1M贴",4100000]
["Y090200098","二极管","1N4007 贴",21152000]
["Y090200029","二极管","SS14 贴",478000]
["Y090200001","二极管","IN4148 贴",300000]
["Y090101017","稳压管","ZMM12V 贴 ",431000]
["Y090101016","稳压管","ZMM5V6 贴 ",1585000]
["Y090200197","稳压管","ZMM10V 贴 ",348000]
["Y080500015","瓷片电容","HCY80F1Y102MW12 ",2533460]
["Y070500048","安规电容","SMD1Y1X1Y5V222M500VAC(Y1 2.2nF ±20% Y5V 500VAC) 贴 ",40000]
["Y070500040","安规电容","X1/Y1223K440VAC 13*12*6 P=10mm L=3.5mm ",40000]
["Y070500039","安规电容","X2 330VAC 15nF ±10% P=10mm L=3.5 插 -40℃～+110℃   ",910032]
["Y070500036","安规电容","22nF/440VAC-X1 P=15mm L=3.5mm",80000]
["Y070500035","安规电容","0.22uF/330VAC-X2 P=15mm 插 L=3.5mm",593120]
["Y070500033","安规电容","X1/Y1104K440VAC 13*8*16 P=10mm L=3.5mm ",710000]
["Y070500031","安规电容","0 .47uF/330VAC 脚间距22.5（长寿命） L=3.5mm",110000]
["Y070500029","安规电容","222M(2.2nF)400V Y1 插  ",128000]
["Y070500017","安规电容","47nF 330V-6*13mm-10mm L=3.5",20605]
["Y070500015","安规电容","0.1uF/330VAC-X2 P=15mm L=3.5mm",1660000]
["Y070500011","安规电容","0.1uF 330VAC P=10mm 厚5mm 插",1687001]
["Y070500009","安规电容","102M(1nF)400V Y1 插",1420000]
["Y051401136","电解电容","ERF1EM681G13B50T 25V 680μF 10*13 L=3.7mm ",150000]
["Y051401127","电解电容","SP 500V 22μF ±20% 13*20 L=3.5mm 插 -25℃～+105℃ ",795000]
["Y051401126","电解电容","SU 400V 22μF ±20% 10.2*20 插 -40℃～+105℃ L=3.7±0.2mm ",80000]
["Y051401115","电解电容","GH 25V 100μF±20% 6.3*11 -40~105℃ L=3.7±0.2mm",195000]
["Y051401114","电解电容","GH 35V 100μF ±20% 6.3*12 插 -40℃～+105℃",41000]
["Y051401109","电解电容","GH 50V 47μF ±20% 6.3*11 插 -40℃～+105℃",714000]
["Y051401105","电解电容","GH 25V 470uF 10*13 插 -40℃～+105℃ L=3.7±0.2mm",2433000]
["Y051401084","电解电容","RS 25V 680μF ±20% 8*20 L=3.7±0.2mm",110000]
["Y051401080","电解电容","HL 450V 15uF 10*20 插  L=3.7±0.2mm",120000]
["Y051401077","电解电容","NXQ 50V 47μF ±20% 6.3*11 插 -40℃～+105℃ L=3.7±0.2mm",230000]
["Y051401075","电解电容","BXC 400V 22uF 12.5*20 L=3.7±0.2mm",1036000]
["Y051401074","电解电容","NXA 25V 220μF ±20% 8*11.5 插 -40℃～+105℃",3570000]
["Y051401072","电解电容","NXA 10V 470uF ±20% L=3.7±0.2mm",425000]
["Y051401058","电解电容","NXA 25V 470uF 8*20（编带）",550000]
["Y051401054","电解电容","NXA 25V 680μF ±20% 8*20 L=3.7±0.2mm 插 -40℃～+105℃",1509000]
["Y051401052","电解电容","NXA 25V 470uF ±20% 8*20 插 -40℃～+105℃ L=8.5±0.2mm 卧式",120000]
["Y051401051","电解电容","NXA 25V 220uF 6.3*11 L=7.5mm 卧式",50000]
["Y051401045","电解电容","NFR 450V 10uF 10*20 L=11",947000]
["Y051401044","电解电容","18uF/400V±20%/KSU/105℃/D*L=10*20(mm)/10000H 脚长L=3.7±0.2mm ",300000]
["Y051401042","电解电容","GH 10V 2200uF 10*20 插 -40℃～+105℃ L=3.7 ±0.2mm",600000]
["Y051401038","电解电容","GH 25V 220uF 6.3*12",260000]
["Y051401036","电解电容","GH 25V 220μF ±20%  8*9  L=3.7±0.2mm 插 -40℃～+105℃ 7000h",40000]
["Y051401027","电解电容","NXA 10V 470uF ±20%",175000]
["Y051401026","电解电容","NXA 25V 470μF ±20% 10*12.5 插 -40℃～+105℃ L=3.7±0.2mm",1509000]
["Y051401024","电解电容","NXA 25V 220μF ±20% 6.3*11 L=3.7±0.2mm 插 -40℃～+105℃",1352000]
["Y051401023","电解电容","NXA 35V 1000μF ±20% 12.5*20 插 -40℃～+105℃ L=3.5±0.5mm",550000]
["Y051401022","电解电容","NFR 450V 10uF L=3.7±0.2mm 10*20",790600]
["Y051401020","电解电容","NXA 10V 220uF ±20% 6.3*11 L=3.7±0.2mm",240000]
["Y051400010","电解电容","NXA 25V 470μF ±20% 8*20 插 -40℃～+105℃",1260000]
["Y051400009","电解电容","NXA 10V 2200μF ±20% 10*20 插 -40℃～+105℃",30000]
["Y051400006","电解电容","NXA 25V 1000μF ±20% 10*20 插 -40℃～+105℃",99026]
["Y051400005","电解电容","NXA 25V 220μF ±20% 6.3*11 插 -40℃～+105℃",4324000]
["Y051400004","电解电容","NXA 35V 1000μF ±20% 12.5*20 插 -40℃～+105℃",1200000]
["Y051200017","电解电容","GH 10V 1000μF ±20% 8*20 插 -40℃～+105℃ L=8.5±0.2mm 卧式",40000]
["Y051200015","电解电容","GH 25V 220uF 20% 8*12 插 -40℃～+105℃ L=4.0±0.2mm",600000]
["Y051100002","电解电容","ZLH 25V 680uF 10*16 L=3.7mm -40℃~+105℃ 插",120000]
["Y050900007","电解电容","SU 450V 10μF ±20% 10*20 L=3.5mm 插 -40℃～+105℃ ",480000]
["Y050900006","电解电容","SP 400V 22μF ±20% 12.5*20 L=3.5mm 插 -40℃～+105℃ ",400000]
["Y050800048","电解电容","YXJ 25V 470uF 10*12.5 L=3.7mm -40℃~+105℃ 插",60000]
["Y050800024","电解电容","YXJ 25V 220μF ±20% 6.3*11 插 -40℃～+105℃",1200000]
["Y050800015","电解电容","YXJ 10V 470uF ±20%",240000]
["Y050800011","电解电容","YXJ 25V 470μF ±20% 10*12.5 插 -40℃～+105℃",480000]
["Y050800002","电解电容","YXJ 25V 1000μF ±20% 10*20 插 -40℃～+105℃",300000]
["Y050205014","电解电容","YXJ 50V 47μF ±20% 6.3*11 插 -40℃～+105℃ ",300000]
["Y050106001","电解电容","BXC 450V 10uF",160000]
["Y990200131","线圈","自粘线圈3523，740uH±20uH， 线径0.15mm ",300000]
["Y990100558","自恢复保险丝","mSMD075-24V 封装1812 贴",40000]
["Y990100295","静电保护器","LESD5Z5.0CT1G 贴 ",400128]
["Y380000031","433MHz弹簧天线","RT433-523W",175000]
["Y380000009","433MHz弹簧天线","RT433-689A",1165645]
["Y990200117","天线","NG-TH-S50 线长3m",552600]
["Y380000004","天线","NG-TH-S61(BC28CNV 24Y023A-11 B5/B8) ",500000]
["Y990100516","4G天线","3A057K",600000]
["Y300200049","容耦隔离器","SP401AW1-DSWR 贴 ",40000]
["Y300200043","耦合变压器","FH9139 插 ",270000]
["Y300200042","耦合变压器","CMC9102 插 ",270000]
["Y300200030","耦合线圈","FH9109 贴 ",100001]
["Y261400042","DC接头端子","DC005-2.0 插",60000]
["Y261400031","USB连接器","Type-C 6pin贴片4脚插母座;触点数量：6P，插脚长2mm，安装方式：卧贴",50000]
["Y260600021","IR46国网物联网表单相电池座","PA66，TFY-LJQ-Z01-001 ",40000]
["Y261400017","接线端子","DG127-5.08-2P ",1282050]
["Y260900251","双排插针","2*9-D2.54mm 双塑塑高2.5mm  一端针长3mm，另一端长8.7mm  中间针长7mm，总长23.7mm",625000]
["Y260900235","双排插针","2*6-D2.54mm 三塑 一头针长3.0mm 另一头头针长10.0mm 90度 中间长24.6mm打弯",175000]
["Y260900187","双排插针","PH2.54MM H2.5MM PC3.0MM PB8.5MM PA7.0MM L18.5MM 2X4PIN 黄铜镀金GF PBT料",175000]
["Y260900174","双排插针","PH2.54 2X8P 蜈蚣脚 H5.0 W12.5(带单柱1.5X1.5)PA10.1 PC3.0 PA6T 镀金2U ",80000]
["Y260900167","双排插针","2*13-D2.54mm，三塑， 短端针长3mm，长端针长6mm 总长39.3mm，第5、6、7、8针去掉,带单个定位柱",20000]
["Y260900156","双排插针","2*8-D2.54mm，双排双塑， 短端针长3mm，长端针长6.5mm 总长19.5mm",320000]
["Y260900146","双排插针","双排90°弯针，2*2-D7.62mm，双塑，一端针长3mm，另一端针长7mm",300000]
["Y260900145","双排插针","2*11-D2.54mm 双塑 一头针长3mm，另一个长9mm  总长 31.5mm",89000]
["Y260900141","双排插针","2*4-D7.62mm 三塑 一头针长3mm，另一头针长6mm，90°打弯",50000]
["Y260900140","双排插针","双排90°弯针，2*6-D2.54mm，双塑，一端针长3mm，另一端针长7mm",300000]
["Y260900116","双排插针","2*13-D2.54mm，三塑， 短端针长3mm，长端针长6mm 总长39.3mm，第5、6、7、8针去掉",120000]
["Y260900111","双排插针","2*4-D2.54mm，双塑， 短端针长3mm，长端针长3mm 总长18mm",800000]
["Y260900108","双排插针","2*4-D2.54mm，三塑， 短端针长3mm，长端针长6mm 总长39.3mm",20000]
["Y260900106","双排插针","2*4-D7.62mm",28000]
["Y260900105","双排插针","2*6-D2.54mm 弯针",503000]
["Y260900097","双排插针","2*4-D2.54mm 双塑 一头针长3mm，另一个长9mm  总长 31.5mm",64025]
["Y260500153","双排插座","2*8-D2.54mm塑高14.5mm(国网单相物联用) 晨翔(DS1023-69) 插",80000]
["Y260500152","双排插座","2*2-D7.62mm塑高26.4mm(O型 PC3.5 PA9T带鱼叉脚触点镀金2μ) ",40000]
["Y260500145","双排插座","BH2.54MM H8.8MM PC3.0MM 2X5PIN 黄铜镀金GF PBT料 电子",300000]
["Y260500118","双排插座","FH:2.54 H:8.5 PC:3.0 2*6P 180度 PA9T O型防漏锡端子，接触点镀金2U 其余部分镀金1U ",300000]
["Y260500117","双排插座","FH:2.54 H:8.5 PC:3.0 2*4P 180度 PA9T 空2.3列 O型防漏锡端子，接触点镀金2U 其余部分镀金1U ",300000]
["Y260500113","双排插座","FH2.54MM H8.5MM PC3.0MM 空7.8.9.11.12列 2X13PIN Y型端子镀金GF PBT料",150000]
["Y260500109","双排插座","FH:2.54 180°2*6P W:5.0 H:7.1 PC:3.2 U型端子防漏锡镀金2U（PBT）",120000]
["Y260500086","双排插座","2*2-D7.62mm，塑高8.5mm",250000]
["Y260500081","双排插座","FH:2.54 180°2*6P W:5.0 H:8.5 PC:3.2 0型端子防漏锡镀金1U（PBT）",630000]
["Y260500080","双排插座","FH:2.54 180度 2*10P 2.3.5.6.8.9列为空位 W:5.0 H:8.5 PC:3.2 0型端子防漏锡镀金1U（PBT）",630000]
["Y260500052","双排插座","2*13-D2.54mm塑高8.5mm ,去掉5、6、7、8针",140000]
["Y260500050","双排插座","2*4-D2.54mm塑高8.5mm",195000]
["Y260500038","双排插座","2*6-D2.54mm塑高7.1mm孔深6.0()",1200000]
["Y260500037","双排插座","2*2-D7.62mm塑高7.1mm孔深6.0()",1200000]
["Y260500034","双排插座","2*6(2.54mm脚间距)塑高8.5 触点距离1.5mm",1684000]
["Y260500026","双排插座","2*4(7.62mm脚间距)触点距离1.5mm",89000]
["Y260500018","双排插座","2*2(脚间距7.62mm)8.5mm高",1345000]
["Y260500009","双排插座","2*8-D2.54mm 塑高8.5mm",320000]
["Y260100148","双排插座","FH2.54MM H8.5MM PC3.0MM 2X19PIN 空7.8.9.11.12.14.15.17.18列 Y型端子镀金GF PBT料 ",25000]
["Y260400029","单排插座","MX3.0-1X3PIN 空第2PIN 电子",300000]
["Y260700105","单排插针","1*2-D5.08mm，门型针，塑高2.5mm，立高21mm（包含塑高），焊脚长4mm",1200000]
["Y260700101","单排插针","1*2-D5.08mm，门型针，塑高3.5mm，立高25.0mm（包含塑高），焊脚长3.5mm，扭15°",250000]
["Y260700091","单排插针","1*2-D5.08mm，门型针，塑高3.5mm，立高23.0mm（包含塑高），焊脚长3.5mm",300000]
["Y260700087","单排插针","1*2-D5.08mm，门型针，塑高2.5mm，立高20mm（包含塑高），焊脚长3mm",40000]
["Y260600030","蜈蚣排母","2*9-D2.54mm 塑高7.1mm 插件 ",625000]
["Y260600023","蜈蚣排母","2*11-D2.54MM 塑高7.1mm 贴片 编带 电子",89000]
["Y260600016","蜈蚣排母","2*4-D2.54MM 塑高7.1mm 贴片 编带",64025]
["Y260200075","排线","蓝白排线  5P, 线长 70mm，一头插针，一头插头 LGG8.510.002",50426]
["Y260100228","插座","5264-2A(直)",210000]
["Y260100137","SMA板座接头","9Z068A-48 ",175000]
["Y260100134","SMA板座接头","92068A-48 ",425000]
["Y260100101","DC直流电源插头插座","DC-002",195000]
["Y260100099","CIU电池插座","HP-2A 直座",1192000]
["Y260100086","插座","5264-2A",1699050]
["Y260100061","插座","8字电源插座(5A 250V)",947000]
["Y260100003","插座","五芯插座",50625]
["Y260100065","RJ45座","RJ45-8P8C",120000]
["Y250100307","变压器电感","YZ3782-EE13 0.2mH ",625000]
["Y250100306","工字电感","LGB0810-103K 10mH ",625000]
["Y250100247","工字电感","DXPK0608-222K-LF  L=3.5±0.5mm",40000]
["Y250100184","工字电感","DXPK0608-472K-LF L=4.5±0.5mm;",250000]
["Y250100182","工字电感","DXPK1012-821K-LF L=4.0",860000]
["Y250100043","工字电感","LGB0608-102K-S3（1mH）",3074000]
["Y250100291","贴片电感","YNR1050-221M ",150000]
["Y250100261","贴片电感","SWPA8040S100MT 贴 ",600000]
["Y250100246","电感","SWPA4018S3R3MT 贴1 ",200000]
["Y250100243","电感","SWPA3015S100MT 贴1 ",200000]
["Y250100236","电感","SWPA4030S220MT 贴 (无锡颖州)",30000]
["Y250100202","电感","SWPA4030S220MT 贴  ",770000]
["Y250100201","电感","SWPA3015S100MT 贴 ",222153]
["Y250100200","电感","SWPA4018S3R3MT 贴 ",2248020]
["Y250100145","电感","CR4018-220M 贴",1790000]
["Y240100042","磁珠","CBG160808U601T 贴 ",600000]
["Y240100040","磁珠","CBG100505U601T",1400000]
["Y240100034","磁珠","470Ω(CBM160808U471T)",425000]
["Y240100033","磁珠","300Ω(CBM160808U301T)",850000]
["Y240100017","磁珠","CBG160808U601T ",300000]
["Y230200015","按键","6*6*5 贴 ",40000]
["Y230100015","按键","6*6*4.3 贴 ",178000]
["Y230200025","触摸弹簧按键","片外径10，总高13(不含引脚)，弹簧外径5.8，引脚长3.5，线径0.4，防锈，单位mm",500000]
["Y230100076","微动开关","KFC781P-4P 7.1*7.1*9.6 插（无极性）",4946000]
["Y230100058","微动开关","KFC581TP-4P(无极性) 贴 ",40000]
["Y230100049","微动开关","PB64N180A-3R ",140000]
["Y220200114","磁阻","1208S 贴 ",1300000]
["Y220200088","磁阻","TMR1362S 贴",700000]
["Y220200085","磁阻","TMR1302S 贴",100000]
["Y040400149","片式电容","0402 50V 6.8nF ±10% X7R 贴 -55℃～+125℃",500000]
["Y040400136","片式电容","0402 50V 2.2nF ±10% NPO 贴 -55℃～+125℃",300000]
["Y040400134","片式电容","0402 16V 0.22μF ±10% X5R 贴 -55℃～+85℃",880000]
["Y040400133","片式电容","0402 50V 0.1μF ±10% X7R 贴 -55℃～+125℃",240000]
["Y040400130","片式电容","0402 50V 4.7nF ±5% X7R 贴 -55℃～+125℃",300000]
["Y040400120","片式电容","0402 50V 1nF ±10% NPO 贴 -55℃～+125℃",1950000]
["Y040400118","片式电容","0402 50V 200pF ±5% NPO 贴 -55℃～+125℃",1400000]
["Y040400093","片式电容","0402 25V 0.47μF ±10% X5R 贴 -55℃～+85℃ (S)",540000]
["Y040400082","片式电容","0402 10V 4.7μF ±10% X5R 贴 -55℃～+85℃ (S)",3200000]
["Y040400081","片式电容","0402 25V 1μF ±10% X5R 贴 -55℃～+85℃(S)",14943000]
["Y040400079","片式电容","0402 25V 33nF X7R ±10% ",5600000]
["Y040400070","片式电容","0402 10V 10μF ±20% X5R 贴 -55℃～+85℃(S)",6180000]
["Y040400068","片式电容","0402 50V 33pF ±5% NP0 贴 -55℃～+125℃",3100000]
["Y040400063","片式电容","0402 10V 2.2μF ±10% X5R 贴 -55℃～+85℃(S)",20000]
["Y040400055","片式电容","0402 25V 0.47μF ±10% X5R 贴 -55℃～+85℃",3300000]
["Y040400054","片式电容","0402 50V 1μF ±10% X5R",240000]
["Y040400053","片式电容","0402 10V 2.2μF ±20% X5R 贴 -55℃～+85℃",500000]
["Y040400052","片式电容","0402 50V 20pF ±5% NP0 贴 -55℃～+125℃",3675000]
["Y040400050","片式电容","0402 50V 47nF ±10% X7R 贴 -55℃～+125℃",10079000]
["Y040400049","片式电容","0402 50V 560pF ±10% X7R 贴 -55℃～+125℃",3120000]
["Y040400046","片式电容","0402 25V 1uF ±10% X5R",200000]
["Y040400027","片式电容","0402 50V 15pF ±5% NP0 贴 -55℃～+125℃",5978000]
["Y040400016","片式电容","0402 50V 10pF ±5% NPO 贴 -55℃～+125℃",2775000]
["Y040400015","片式电容","0402 50V 3.3nF ±10% X7R 贴 -55℃～+125℃",240000]
["Y040400012","片式电容","0402 50V 220pF ±5%",4800000]
["Y040400009","片式电容","0402 16V 0.1μF ±10% X7R 贴 -55℃～+125℃",18260000]
["Y040400008","片式电容","0402 50V 0.01μF ±10% X7R 贴 -55℃～+125℃",73284000]
["Y040400007","片式电容","0402 50V 1nF ±10% X7R 贴 -55℃～+125℃",6906128]
["Y040400005","片式电容","0402 50V 100pF ±5% NP0 贴 -55℃～+125℃",16885000]
["Y040400004","片式电容","0402 50V 22pF ±5% NP0 贴 -55℃～+125℃",1020000]
["Y040400001","片式电容","0402 25V 0.1μF ±10% X7R 贴 -55℃～+125℃",92124000]
["Y040300067","片式电容","1206 1000V 100pF ±5% NP0 贴 -55℃～+125℃",320000]
["Y040300065","片式电容","1206 2000V 1nF ±5% X7R 贴 -55℃～+125℃",150000]
["Y040300049","片式电容","1206 1kV 470pF ±10% X7R",1580000]
["Y040300038","片式电容","1206 1kV 2.2nF ±10% X7R 贴 -55℃～+125℃",688000]
["Y040300037","片式电容","1206 1000V 0.01μF ±10% X7R 贴 -55℃～+125℃",2065000]
["Y040300036","片式电容","1206 1000V 47pF ±5% NP0 贴 -55℃～+125℃",1139400]
["Y040300029","片式电容","1206 1kV 2.2nF ±10%",40000]
["Y040300013","片式电容","1206 1000V 1nF ±10% X7R 贴 -55℃～+125℃",80000]
["Y040201156","片式电容","0603 25V 22nF ±10% X7R 贴 -55℃～+125℃",40000]
["Y040201155","片式电容","0603 50V 0.22μF ±10% X7R 贴 -55℃～+125℃",1372000]
["Y040201139","片式电容","0603 50V 2.2μF ±10% X5R 贴 -55℃～+85℃ (S)",1750000]
["Y040201138","片式电容","0603 50V 1μF ±10% X5R 贴 -55℃～+85℃(S)",625000]
["Y040201135","片式电容","0603 25V 1μF ±10% X7R 贴 -55℃～+125℃(S)",971050]
["Y040201134","片式电容","0603 25V 1μF ±10% X5R 贴 -55℃～+85℃(S)",725000]
["Y040201133","片式电容","0603 25V 10μF ±20% X5R 贴 -55℃～+85℃(S)",23677025]
["Y040201132","片式电容","0603 10V 4.7μF ±10% X5R 贴 -55℃～+85℃(S)",60000]
["Y040201129","片式电容","0603 10V 10μF ±20% X5R 贴 -55℃～+85℃(S)",7435128]
["Y040201121","片式电容","0603 10V 22uF",4825000]
["Y040201107","片式电容","0603 50V 22nF ±10% X7R 贴 -55℃～+125℃",690000]
["Y040201082","片式电容","0603 25V 0.1μF ±10% X7R 贴 -55℃～+125℃",930000]
["Y040201080","片式电容","0603 50V 47nF ±10% X7R 贴 -55℃～+125℃",830000]
["Y040201038","片式电容","0603 10V 10μF ±20% X5R 贴 -55℃～+85℃",16480000]
["Y040201036","片式电容","0603 25V 0.22μF ±10% X7R 贴 -55℃～+125℃",830000]
["Y040201034","片式电容","0603 25V 10μF ±20% X5R 贴 -55℃～+85℃",100000]
["Y040201031","片式电容","0603 10V 4.7μF ±10% X5R 贴 -55℃～+85℃",8750000]
["Y040201030","片式电容","0603 10V 2.2uF ±10% X5R 贴 -55℃～+85℃",1750000]
["Y040201025","片式电容","0603 25V 1μF ±10% X5R 贴 -55℃～+85℃",11420000]
["Y040201019","片式电容","0603 50V 1μF ±10% X5R 贴 -55℃～+85℃",3580000]
["Y040201018","片式电容","0603 25V 0.47μF ±10% X7R 贴 -55℃～+125℃",955000]
["Y040201017","片式电容","0603 50V 0.01μF ±10% X7R 贴 -55℃～+125℃",150000]
["Y040201016","片式电容","0603 50V 0.1μF ±10% X7R 贴 -55℃～+125℃",2362075]
["Y040201014","片式电容","0603 50V 33nF ±10% X7R 贴 -55℃～+125℃",23471000]
["Y040201011","片式电容","0603 50V 2.2nF ±10% X7R 贴 -55℃～+125℃",790000]
["Y040201009","片式电容","0603 50V 1nF ±10% X7R 贴 -55℃～+125℃",40010]
["Y040101106","片式电容","0805 500V 100pF ±5% X7R 贴 -55℃～+125℃",140050]
["Y040101102","片式电容","0805 500V 470pF ±10% X7R 贴 -55℃～+125℃",1393000]
["Y040101088","片式电容","0805 25V 10μF ±10% X5R 贴 -55℃～+85℃(S)",2600000]
["Y040101080","片式电容","0805 50V 4.7uF X5R",1918075]
["Y040101077","片式电容","0805 25V 1μF ±10% X7R 贴 -55℃～+125℃",1580000]
["Y040101075","片式电容","0805 25V 10μF ±10% X5R 贴 -55℃～+85℃",1876000]
["Y040101064","片式电容","0805 10V 22μF ±20% X5R 贴 -55℃～+85℃（S）",100000]
["Y040101049","片式电容","0805 50V 4.7nF ±10% X7R 贴 -55℃～+125℃",779000]
["Y030204033","热敏电阻","SPMZ11-06E151-251R/10D431  L=3.5mm 2B",1884000]
["Y030204032","热敏电阻","SPMZ11-19E050-080RM L=3.5mm",30000]
["Y030201105","热敏电阻","MZ11-06E201-401RM/10D391  L=3.5mm 3A",1500000]
["Y030201104","热敏电阻","MZ11-10A(300-600)RM  L=3.5 450",4053050]
["Y030201101","热敏电阻","MZ11-06E800-161RM/10D391 L=3.5 ",80000]
["Y030201100","热敏电阻","SPMZ11-06E151-251R/10D431()",748000]
["Y030201099","热敏电阻","MZ11-06E201-401RM/10D391  L=3.5mm",250000]
["Y030201032","热敏电阻","MZ11-10A(300-600)RM  L=3.5",442400]
["Y030201022","热敏电阻","MZ11 06A(300-600)RM ",100010]
["Y030101011","热敏电阻","MZ11-10A(300-600)RM L=3.5mm ",200000]
["Y020800051","绕线电阻","3W ±5% 22Ω（防浪涌、立式直角成型）加热缩管  ",40000]
["Y020800027","绕线电阻","RXF21-3W-220R-J(立式成型) 插 ",110000]
["Y020800026","绕线电阻","3W ±5% 75Ω（防浪涌、立式直角成型、脚间距8.5mm）加热缩管",630000]
["Y020800016","绕线电阻","RXF21-3W-47Ω-J 立式成型 插 ",388000]
["Y020800014","绕线电阻","RXF21-3W-22Ω-J(卧式内K) 插 ",444000]
["Y020800009","绕线电阻","3W ±5% 22Ω（防浪涌、立式直角成型）",2155000]
["Y020100031","无引线色环电阻","0204 1/4W ±1% 5.1Ω ≤25ppm",956000]
["Y011200005","无引线色环电阻","0207 100K ±1% 1W 50ppm",550000]
["Y010500054","无引线色环电阻","MMA02040C2003FB300 0204 ±1% 1/4W 200kΩ ±50ppm ",720000]
["Y010500039","无引线色环电阻","CSRA系列 0204 ±1% 1/4W 10Ω ≤25ppm ",180000]
["Y010500038","无引线色环电阻","CSRA系列 0204 ±1% 1/4W 5.1Ω ≤25ppm ",3980000]
["Y010500034","无引线色环电阻","CSRA系列 0204 ±1% 1/4W 51kΩ ≤25ppm ",720000]
["Y010500033","无引线色环电阻","CSRA系列 0204 ±1% 1/4W 100kΩ ≤25ppm ",800000]
["Y010500032","无引线色环电阻","CSRA系列 0204 ±1% 1/4W 200kΩ ≤25ppm ",14720000]
["Y010500021","无引线色环电阻","0204 ±1% 2Ω 1/4W ≤50ppm",480000]
["Y010500016","无引线色环电阻","0204 ±1% 5.1Ω  1/4W ≤50ppm ",40000]
["Y010102136","片式电阻","RAM05FTCW1001 0805 ±1% 1/8W 1kΩ ≤25ppm ",8160000]
["Y010102134","片式电阻","RAM05FTCW1503 0805 ±1% 1/8W 150kΩ ≤25ppm ",11600000]
["Y010102129","片式电阻","RAM05FTCW1201 0805 ±1% 1/8W 1.2kΩ ≤25ppm ",4180000]
["Y010102128","片式电阻","RAM05FTCW0360 0805 ±1% 1/8W 36Ω ≤25ppm ",3500000]
["Y010102127","片式电阻","RAM05FTCW1500 0805 ±1% 1/8W 150Ω ≤25ppm ",1100000]
["Y010102126","片式电阻","RAM05FTCW2003 0805 ±1% 1/8W 200kΩ ≤25ppm ",2400000]
["Y010202132","片式电阻","RAM06FTCV3303 1206 ±1% 1/4W 330kΩ ≤25ppm ",810000]
["Y010302168","片式电阻","RAM0603 ±1% 1.2kΩ 1/10W ±25ppm 贴 -55℃～+155℃",1960000]
["Y010302163","片式电阻","RAM03FTCX1001 0603 ±1% 1/10W 1kΩ ≤25ppm ",5980000]
["Y010302082","片式电阻","0603 ±1% 1Ω 1/10W ±25ppm 贴 -55℃～+155℃",200000]
["Y010302077","片式电阻","0603 ±1% 1kΩ 1/10W ±25ppm 贴 -55℃～+155℃",1100000]
["Y010302075","片式电阻","0603 ±1% 1.2kΩ 1/10W ±25ppm 贴 -55℃～+155℃",7604000]
["Y010102077","片式电阻","0805 ±1% 1kΩ 1/8W ±25ppm 贴 -55℃～+155℃",148000]
["Y010900101","片式电阻","0402 ±1% 5.1kΩ  1/16W ±100ppm 贴 -55℃～+155℃",800000]
["Y010900100","片式电阻","0402 ±1% 1MΩ 1/16W ±100ppm 贴 -55℃～+155℃",450000]
["Y010900099","片式电阻","0402 ±1% 7.5kΩ 1/10W ±100ppm 贴 -55℃～+155℃",800000]
["Y010900071","片式电阻","0402 ±1% 30kΩ 1/16W ±100ppm 贴 -55℃～+155℃",910000]
["Y010900067","片式电阻","0402 ±1% 115kΩ 1/16W ±100ppm 贴 -55℃～+155℃",440000]
["Y010900048","片式电阻","0402 ±1% 1.2kΩ 1/16W ±100ppm 贴 -55℃～+155℃",830000]
["Y010900042","片式电阻","0402 ±1% 5.1kΩ ±50ppm ",678000]
["Y010900041","片式电阻","0402 ±1% 1.5kΩ 1/16W ±100ppm 贴 -55℃～+155℃",600000]
["Y010900039","片式电阻","0402 ±1% 240KΩ",305000]
["Y010900038","片式电阻","0402 ±1% 100kΩ 1/16W ±100ppm 贴 -55℃～+155℃",9117120]
["Y010900037","片式电阻","0402 ±1% 510Ω",231025]
["Y010900033","片式电阻","0402 ±1% 300kΩ 1/16W ±100ppm 贴 -55℃～+155℃",3127128]
["Y010900031","片式电阻","0402 ±1% 47kΩ 1/16W ±100ppm 贴 -55℃～+155℃",546425]
["Y010900030","片式电阻","0402 ±1% 24kΩ 1/16W ±100ppm 贴 -55℃～+155℃",80000]
["Y010900029","片式电阻","0402 ±1% 22kΩ 1/16W ±100ppm 贴 -55℃～+155℃",735000]
["Y010900027","片式电阻","0402 ±1% 20kΩ 1/16W ±100ppm 贴 -55℃～+155℃",6354000]
["Y010900024","片式电阻","0402 ±1% 10MΩ 1/16W ±100ppm 贴 -55℃～+155℃",1080000]
["Y010900022","片式电阻","0402 ±1% 1M 1/16W ±100ppm 贴 -55℃～+155℃",1877000]
["Y010900021","片式电阻","0402 ±1% 2MΩ 1/16W ±100ppm 贴 -55℃～+155℃",4294128]
["Y010900020","片式电阻","0402 ±1% 200kΩ 1/16W ±100ppm 贴 -55℃～+155℃",2409000]
["Y010900019","片式电阻","0402 ±1% 220kΩ 1/16W ±100ppm 贴 -55℃～+155℃",1750000]
["Y010900018","片式电阻","0402 ±1% 120kΩ 1/16W ±100ppm 贴 -55℃～+155℃",3150000]
["Y010900017","片式电阻","0402 ±1% 36kΩ 1/16W ±100ppm 贴 -55℃～+155℃",2380000]
["Y010900016","片式电阻","0402 ±1% 15kΩ 1/16W ±100ppm 贴 -55℃～+155℃",2427000]
["Y010900015","片式电阻","0402 ±1% 11kΩ 1/16W ±100ppm 贴 -55℃～+155℃",1510000]
["Y010900014","片式电阻","0402 ±1% 100Ω 1/16W ±100ppm 贴 -55℃～+155℃",300000]
["Y010900013","片式电阻","0402 ±1% 51kΩ 1/16W ±100ppm 贴 -55℃～+155℃",3653000]
["Y010900012","片式电阻","0402 ±1% 33kΩ 1/16W ±100ppm 贴 -55℃～+155℃",1680000]
["Y010900008","片式电阻","0402 ±1% 82k 1/16W ±100ppm 贴 -55℃～+155℃",420148]
["Y010900007","片式电阻","0402 ±1% 10kΩ 1/16W ±100ppm 贴 -55℃～+155℃",21699473]
["Y010900005","片式电阻","0402 ±1% 4.7kΩ 1/16W ±100ppm 贴 -55℃～+155℃",144000]
["Y010900002","片式电阻","0402 ±1% 12kΩ 1/16W ±100ppm 贴 -55℃～+155℃",60000]
["Y010600057","片式电阻","0402 ±5% 33kΩ 1/16W ±100ppm 贴 -55℃～+155℃",230000]
["Y010600054","片式电阻","0402 ±5% 22Ω 1/16W ±100ppm 贴 -55℃～+155℃",1500000]
["Y010600051","片式电阻","0402 ±5% 47kΩ 1/16W ±100ppm 贴 -55℃～+155℃",1350000]
["Y010600050","片式电阻","0402 ±5% 510kΩ 1/16W ±100ppm 贴 -55℃～+155℃",2972000]
["Y010600049","片式电阻","0402 ±5% 680Ω 1/16W ±100ppm 贴 -55℃～+155℃",10559010]
["Y010600042","片式电阻","0402 ±5% 200Ω 1/16W ±100ppm 贴 -55℃～+155℃",2744000]
["Y010600039","片式电阻","0402 ±5% 10M 1/16W ±100ppm 贴 -55℃～+155℃",3150000]
["Y010600038","片式电阻","0402 ±5% 1.5MΩ 1/16W ±100ppm 贴 -55℃～+155℃",710000]
["Y010600036","片式电阻","0402 ±5% 3MΩ 1/16W ±100ppm 贴 -55℃～+155℃",170000]
["Y010600035","片式电阻","0402 ±5% 300kΩ 1/16W ±100ppm 贴 -55℃～+155℃",630000]
["Y010600034","片式电阻","0402 ±5% 200kΩ 1/16W ±100ppm 贴 -55℃～+155℃",1045025]
["Y010600033","片式电阻","0402 ±5% 5.1kΩ 1/16W ±100ppm 贴 -55℃～+155℃",32483425]
["Y010600032","片式电阻","0402 ±1% 150kΩ 1/16W ±100ppm 贴 -55℃～+155℃",1750000]
["Y010600026","片式电阻","0402 ±5% 4.7kΩ 1/16W ±100ppm 贴 -55℃～+155℃",4860000]
["Y010600024","片式电阻","0402 ±5% 0Ω 贴 -55℃～+155℃",5240000]
["Y010600022","片式电阻","0402 ±5% 3kΩ 1/16W ±100ppm 贴 -55℃～+155℃",3000000]
["Y010600019","片式电阻","0402 ±5% 300Ω 1/16W ±100ppm 贴 -55℃～+155℃",1156020]
["Y010600018","片式电阻","0402 ±5% 1kΩ 1/16W ±100ppm 贴 -55℃～+155℃",70741000]
["Y010600017","片式电阻","0402 ±5% 100Ω 1/16W ±100ppm 贴 -55℃～+155℃",78477000]
["Y010600016","片式电阻","0402 ±5% 1MΩ 1/16W ±100ppm 贴 -55℃～+155℃",13162020]
["Y010600015","片式电阻","0402 ±5% 470kΩ 1/16W ±100ppm 贴 -55℃～+155℃",270000]
["Y010600012","片式电阻","0402 ±5% 100kΩ 1/16W ±100ppm 贴 -55℃～+155℃",22300425]
["Y010600011","片式电阻","0402 ±5% 51kΩ 1/16W ±100ppm 贴 -55℃～+155℃",4902000]
["Y010600010","片式电阻","0402 ±5% 20kΩ 1/16W ±100ppm 贴 -55℃～+155℃",15646560]
["Y010600009","片式电阻","0402 ±5% 10kΩ 1/16W ±100ppm 贴 -55℃～+155℃",95030000]
["Y010600007","片式电阻","0402 ±5% 2kΩ 1/16W ±100ppm 贴 -55℃～+155℃",12684020]
["Y010600004","片式电阻","0402 ±5% 510Ω 1/16W ±100ppm 贴 -55℃～+155℃",9249000]
["Y010600002","片式电阻","0402 ±5% 51Ω 1/16W ±100ppm 贴 -55℃～+155℃",11480000]
["Y010600001","片式电阻","0402 ±5% 10Ω 1/16W ±200ppm 贴 -55℃～+155℃",22785000]
["Y010302214","片式电阻","0603 ±1% 360Ω 1/10W ±25ppm 贴 -55℃～+155℃",2865000]
["Y010302203","片式电阻","0603 ±1% 2Ω 1/10W ±25ppm 贴 -55℃～+155℃",400000]
["Y010302086","片式电阻","0603 ±1% 5.1Ω 1/10W ±50ppm 贴 -55℃～+155℃",2770010]
["Y010302069","片式电阻","0603 ±1% 20kΩ 1/10W ±100ppm 贴 -55℃～+155℃",88000]
["Y010302065","片式电阻","0603 ±1% 30kΩ 1/10W ±100ppm 贴 -55℃～+155℃",30000]
["Y010302062","片式电阻","0603 ±1% 33kΩ 1/10W ±100ppm 贴 -55℃～+155℃",710000]
["Y010302050","片式电阻","0603 ±1% 7.5kΩ 1/10W ±100ppm 贴 -55℃～+155℃",630000]
["Y010302044","片式电阻","0603 ±1% 22kΩ 1/10W ±100ppm 贴 -55℃～+155℃",25000]
["Y010302041","片式电阻","0603 ±1% 100Ω 1/10W ±100ppm 贴 -55℃～+155℃",600000]
["Y010302040","片式电阻","0603 ±1% 18kΩ 1/10W ±100ppm 贴 -55℃～+155℃",948000]
["Y010302033","片式电阻","0603 ±1% 51kΩ 1/10W ±100ppm 贴 -55℃～+155℃",40000]
["Y010302030","片式电阻","0603 ±1% 10kΩ 1/10W ±100ppm 贴 -55℃～+155℃",120000]
["Y010302026","片式电阻","0603 ±1% 2kΩ 1/10W ±100ppm 贴 -55℃～+155℃",40000]
["Y010302019","片式电阻","0603 ±1% 39kΩ 1/10W ±100ppm 贴 -55℃～+155℃",50000]
["Y010302012","片式电阻","0603 ±1% 4.7kΩ 1/10W ±100ppm 贴 -55℃～+155℃",1218000]
["Y010302011","片式电阻","0603 ±1% 1.2kΩ 1/10W ±100ppm 贴 -55℃～+155℃",1232000]
["Y010302010","片式电阻","0603 ±1% 5.1Ω 1/10W ±200ppm 贴 -55℃～+155℃",3588000]
["Y010302007","片式电阻","0603 ±1% 1kΩ 1/10W ±100ppm 贴 -55℃～+155℃",173000]
["Y010302003","片式电阻","0603 ±1% 330Ω 1/10W ±100ppm 贴 -55℃～+155℃",410000]
["Y010301078","片式电阻","0603 ±5% 22Ω 1/10W ±100ppm 贴 -55℃～+155℃",600000]
["Y010301065","片式电阻","0603 ±5% 2MΩ 1/10W ±100ppm 贴 -55℃～+155℃",310000]
["Y010301051","片式电阻","0603 ±5% 200Ω 1/10W ±100ppm 贴 -55℃～+155℃",40000]
["Y010301039","片式电阻","0603 ±5% 47kΩ 1/10W ±100ppm 贴 -55℃～+155℃",830000]
["Y010301033","片式电阻","0603 ±5% 20kΩ 1/10W ±100ppm 贴 -55℃～+155℃",845050]
["Y010301029","片式电阻","0603 ±5% 10kΩ 1/10W ±100ppm 贴 -55℃～+155℃",320000]
["Y010301019","片式电阻","0603 ±5% 2kΩ 1/10W ±100ppm 贴 -55℃～+155℃",1016000]
["Y010301018","片式电阻","0603 ±5% 1.2kΩ 1/10W ±100ppm 贴 -55℃～+155℃",60000]
["Y010301017","片式电阻","0603 ±5% 1kΩ 1/10W ±100ppm 贴 -55℃～+155℃",1594000]
["Y010301014","片式电阻","0603 ±5% 510Ω 1/10W ±100ppm 贴 -55℃～+155℃",3450000]
["Y010301013","片式电阻","0603 ±5% 330Ω 1/10W ±100ppm 贴 -55℃～+155℃",1025000]
["Y010301012","片式电阻","0603 ±5% 300Ω 1/10W ±100ppm 贴 -55℃～+155℃",1500000]
["Y010301011","片式电阻","0603 ±5% 240Ω 1/10W ±100ppm 贴 -55℃～+155℃",4754000]
["Y010301007","片式电阻","0603 ±5% 100Ω 1/10W ±100ppm 贴 -55℃～+155℃",290000]
["Y010301006","片式电阻","0603 ±5% 51Ω 1/10W ±100ppm 贴 -55℃～+155℃",90000]
["Y010301005","片式电阻","0603 ±5% 20Ω 1/10W ±100ppm 贴 -55℃～+155℃",710000]
["Y010301004","片式电阻","0603 ±5% 10Ω 1/10W ±200ppm 贴 -55℃～+155℃",7513000]
["Y010301001","片式电阻","0603 ±5% 0Ω 1/10W 贴 -55℃～+155℃",4295173]
["Y010202129","片式电阻","1206 ±1% 2Ω 1/4W ±200ppm 贴 -55℃～+155℃",1600000]
["Y010202115","片式电阻","1206 ±1% 820kΩ 1/4W ±100ppm 200V 贴 -55℃～+155℃",149000]
["Y010202100","片式电阻","1206 ±1% 240K",352000]
["Y010202077","片式电阻","1206 ±1% 51kΩ 1/4W ±50ppm 贴 -55℃～+155℃",960000]
["Y010202054","片式电阻","1206 ±1% 20kΩ 1/4W ±10ppm 贴 -55℃～+155℃",120050]
["Y010202048","片式电阻","1206 ±1% 2MΩ 1/4W ±100ppm 贴 -55℃～+155℃",4059000]
["Y010202047","片式电阻","1206 ±1% 1MΩ 1/4W ±100ppm 贴 -55℃～+155℃",3846000]
["Y010202043","片式电阻","1206 ±1% 330kΩ 1/4W ±25ppm 贴 -55℃～+155℃",2928000]
["Y010202035","片式电阻","1206 ±1% 200kΩ 1/4W ±25ppm 贴 -55℃～+155℃",13380000]
["Y010202032","片式电阻","1206 ±1% 1kΩ 1/4W ±100ppm 贴 -55℃～+155℃",1954128]
["Y010202026","片式电阻","1206 ±1% 120kΩ 1/4W ±100ppm 贴 -55℃～+155℃",4156050]
["Y010202017","片式电阻","1206 ±1% 470kΩ 1/4W ±100ppm 贴 -55℃～+155℃",4186000]
["Y010202010","片式电阻","1206 ±1% 150kΩ 1/4W ±100ppm 贴 -55℃～+155℃",1200000]
["Y010201041","片式电阻","1206 ±5% 4.7kΩ 1/4W ±100ppm 贴 -55℃～+155℃",310000]
["Y010201031","片式电阻","1206 ±5% 1kΩ 1/4W ±100ppm 贴 -55℃～+155℃",999445]
["Y010201030","片式电阻","1206 ±5% 200Ω 1/4W ±100ppm 贴 -55℃～+155℃",356095]
["Y010201021","片式电阻","1206 ±5% 2Ω 1/4W ±200ppm 贴 -55℃～+155℃",1204000]
["Y010201020","片式电阻","1206 ±5% 1Ω 1/4W ±200ppm 贴 -55℃～+155℃",1284000]
["Y010201019","片式电阻","1206 ±5% 51Ω 1/4W ±100ppm 贴 -55℃～+155℃",4895000]
["Y010201018","片式电阻","1206 ±5% 10Ω 1/4W ±200ppm 贴 -55℃～+155℃",1976000]
["Y010201013","片式电阻","1206 ±5% 20Ω 1/4W ±100ppm 贴 -55℃～+155℃",2784400]
["Y010201008","片式电阻","1206 ±5% 51kΩ 1/4W ±100ppm 贴 -55℃～+155℃",480000]
["Y010201007","片式电阻","1206 ±5% 0Ω 贴 -55℃～+155℃",1026200]
["Y010201005","片式电阻","1206 ±5% 470kΩ 1/4W ±100ppm 贴 -55℃～+155℃",888000]
["Y010201001","片式电阻","1206 ±5% 100kΩ 1/4W ±100ppm 贴 -55℃～+155℃",172000]
["Y010102069","片式电阻","0805 ±1% 120kΩ",20000]
["Y010102056","片式电阻","0805 ±1% 390kΩ 1/8W ±100ppm 贴 -55℃～+155℃",1500000]
["Y010102051","片式电阻","0805 ±1% 200kΩ 1/8W ±100ppm 贴 -55℃～+155℃",1000000]
["Y010102049","片式电阻","0805 ±1% 150kΩ 1/8W ±100ppm 贴 -55℃～+155℃",6000000]
["Y010102045","片式电阻","0805 ±1% 51kΩ 1/8W ±100ppm 贴 -55℃～+155℃",250000]
["Y010102038","片式电阻","0805 ±1% 20kΩ",20000]
["Y010102017","片式电阻","0805 ±1% 510Ω",947000]
["Y010102016","片式电阻","0805 ±1% 470Ω 1/8W ±100ppm 贴 -55℃～+155℃",100000]
["Y010102008","片式电阻","0805 ±1% 10Ω 1/8W ±200ppm 贴 -55℃～+155℃",200000]
["Y010101041","片式电阻","0805 ±5% 10kΩ 1/8W ±100ppm 贴 -55℃～+155℃",300000]
["Y010101031","片式电阻","0805 ±5% 3kΩ 1/8W ±100ppm 贴 -55℃～+155℃",80000]
["Y010101027","片式电阻","0805 ±5% 1.5kΩ 1/8W ±100ppm 贴 -55℃～+155℃",790000]
["Y010101025","片式电阻","0805 ±5% 1kΩ 1/8W ±100ppm 贴 -55℃～+155℃",1230000]
["Y010101009","片式电阻","0805 ±5% 51Ω 1/8W ±100ppm 贴 -55℃～+155℃",4930000]
["Y010101006","片式电阻","0805 ±5% 20Ω 1/8W ±100ppm 贴 -55℃～+155℃",2370000]
["Y010101005","片式电阻","0805 ±5% 10Ω 1/8W ±200ppm 贴 -55℃～+155℃",1420000]
["J570300127","不干胶贴纸","消银龙不干胶贴纸，防水，带背胶，尺寸：25*6mm，带印字，图号：LGG0.860.160D-01 ",20000]
["J570300046","标签纸","42*12 普通单排（内纸筒40mm）自动贴标机专用 ",1260000]
["J570300033","易碎品标签贴纸","英文版，警示贴纸，90*75mm，不干胶铜版纸，图号：LGG0.860.014",16633]
["J52200281","密封圈","硅胶材质，与机芯配套使用，图纸：JS-LLW-12-147C",100000]
["J52200231","磁钢（红色指针）","配套于中间采样机芯（霍尔采样），安装孔配直径为1.7的齿轮柱，指针总高度6.2mm，图号：JS-LLW-12-167A",800000]
["J52200210","密封垫","PVC材质，图纸：JS-LLW-12-148A",800000]
["J52200209","密封圈","橡胶材质，与机芯配套使用，图纸：JS-LLW-12-147B",700000]
["J52200205","不锈钢罩","不锈钢材质，与铜壳配套，外径75mm，中孔62mm",800000]
["J52200029","玻璃","Φ70*6",800000]
["J520603138","止回阀","DN25（不锈钢材质，进水端安装，螺纹参数图号NG8.863.GJT-XTBN)",800000]
["J520603137","止回阀","DN20（不锈钢材质，进水端安装，螺纹参数图号NG8.863.GJT-XTBN)",800000]
["J520603123","止回阀","DN15（不锈钢材质，进水端安装，螺纹参数图号NG8.863.GJT-XTBN)",800000]
["J520603068","止回阀","DN20 进水端安装，螺纹参数图号NG8.863.GJT-XTBN",800000]
["J520603066","止回阀","DN15 进水端安装，螺纹参数图号NG8.863.GJT-XTBN",800000]
["J520200162","止回阀","DN25 铜材质，进水端安装，螺纹参数图号NG8.863.GJT-XTBN",800000]
["J520200153","连接螺母","DN25 不锈钢材质，内螺纹",800000]
["J520200152","连接螺母","DN20 不锈钢材质，内螺纹",800000]
["J520200151","连接螺母","DN15 不锈钢材质，内螺纹",800000]
["J520200071","连接螺母","DN25(铜质，内螺纹)",800000]
["J520200068","连接螺母","DN15(铜质，内螺纹)",800000]
["J520200066","连接螺母","DN20(铜质，内螺纹)",800000]
["J520200150","管接头","DN25 不锈钢材质，单侧外螺纹  管接头图号：NG8.863.GJT-XTBN",800000]
["J520200149","管接头","DN20 不锈钢材质，单侧外螺纹  管接头图号：NG8.863.GJT-XTBN",800000]
["J520200148","管接头","DN15 不锈钢材质，单侧外螺纹  管接头图号：NG8.863.GJT-XTBN",800000]
["J520200070","管接头","DN25(铜质，单侧外螺纹)",800000]
["J520200067","管接头","DN15(铜质，单侧外螺纹)",800000]
["J520200065","管接头","DN20(铜质，单侧外螺纹)",800000]
["J520200076","水表一拉锁","DN15",800000]
["J460300376","防磁板","铁，表面喷塑，黑色（绝缘），厚度2mm，尺寸：108*82mm，符合RoHS，图号：LGG8.610.362K-01",60000]
["J460300259","硅胶按键","硅胶按键，硅橡胶，白色，12位，5号带盲点，确认键为红色，44.5*40.5*12.3mm,图号：LGG8.730.540K-02 ",420000]
["J460300232","硅胶按键","硅胶按键，硅橡胶，白色，12位，5号带盲点，确认键为蓝色，45.4*41.4*21mm，图号：LGG8.730.360K-01",50000]
["J460300231","硅胶按键","硅胶按键，硅橡胶，白色，12位，5号带盲点，确认键为蓝色，44.5*40.5*10mm,图号：LGG8.730.540K-01",250000]
["J460300230","接线端子套","10.6×13×15.7mm，H62铜，镀镍，LGG8.585.006",481000]
["J460300364","接线端子套","9×10.4×20.2mm，铜，镀镍，符合RoHS，图号：LGG8.585.162K-01",1020000]
["J460300225","接线端子套","10.6×13×15.7mm，铁，镀环保彩锌，LGG8.585.006",800000]
["J460300220","接线端子套","9.1×11.6×16mm，H62铜，镀镍，LGG8.585.005",4208000]
["J460300214","接线端子套","18.5×12×15.5mm，铁，镀三价铬彩锌，LGG8.585.001",496000]
["J460300206","接线端子套","9.1×11.6×16mm，铁，镀彩锌，LGG8.585.005",620000]
["J460300057","接线端子套组件","接线端子套（LGG8.585.004）配M7×13.5螺钉，16.6×13×10.5mm，铁，镀彩锌，组件图号：LGG5.585.004",80000]
["J460300129","电流接线端片","T2铜，31×29×2mm，酸洗，LGG8.522.100-01",10000]
["J460300118","硅胶按键","硅橡胶，带碳膜，白色，尺寸7.8*7mm，图号：LGG8.730.006",20000]
["J460300059","防水接头","M30*1.5，白色，PA66，IP68",800000]
["J460300056","导光柱","导光柱，PC，透明，LGG8.770.002",140000]
["J460300053","铅封","塑料铅封，PC+GF10+FR，红色，LGG8.870.002",24000]
["J460300015","铅封","铝管铅封，纯铝，φ4×10mm，LGG8.870.001",881000]
["J370400018","铅封豆","嵌入式 新规范",1020000]
["J370400017","铅封豆","嵌入式(南网专用)",950000]
["J240100005","铅封丝","长度83mm（2根铜丝1根钢丝缠绕）",1117000]
["J230100110","塑料铅封","塑料铅封，PC+GF10+FR，蓝色 PANTONE 293C，LGG8.870.160K-B1",100000]
["J230100109","塑料铅封","塑料铅封，PC+GF10+FR，无LOGO，红色，LGG8.870.004",940000]
["J230100099","铝皮铅封","材质：聚碳酸酯，厚度5.5mm，直径15.5mm，铝皮黑色，无印字",36000]
["J230100080","铅封豆","材质：铅，尺寸：φ10*4mm",200000]
["J230100025","铅封豆","嵌入式 新规范正泰",1200000]
["J210700080","机牙螺丝","M2.5*8（盘头螺丝，不锈钢，复合槽）",800000]
["J210700070","机牙螺丝","KM2.5*10 不锈钢，沉头，十字槽",3200000]
["J210700035","机牙螺丝","PM3*55(不锈钢 圆头 复合槽)",3200000]
["J210401017","三组合螺钉","复合槽盘头螺钉、平垫和弹垫组合件，铁镀彩锌，M4*40， 标准JIS B 1188 (T1A)-1995",174000]
["J300300300","端钮螺丝","M5*11，复合槽，中碳钢镀三价铬环保彩锌，硬化处理，JS-DDG-03-004",16000000]
["J300300206","端钮螺丝","M6*12；复合槽；铜镀镍",8200000]
["J210301050","自攻螺钉","小沉头自攻螺钉，ST2.8*8，头径3.6mm，碳钢镀彩锌",1005000]
["J210301044","自攻螺钉","ST2.9*16(平尾F型，不锈钢，十字槽，盘头)",2800000]
["J210301031","自攻螺钉","ST2.9*8（沉头），十字槽，铁镀彩锌，头部直径6mm",76000]
["J210301027","自攻螺钉","ST2.9*6（铁，镀彩锌，十字槽，盘头，GB 845-85）",100000]
["J210202107","铅封螺钉","M4×40，铁，镀环保彩锌，复合槽，四孔，符合RoHS，图号：LGG8.910.001",360000]
["J210202101","铅封螺钉","M4×20，铁，镀彩锌，内三角槽，四孔，图号：LGG8.910.006",21000]
["J300300104","铅封螺钉","NW-M4*20(复合槽 不锈钢四孔穿线式南网专用)",550000]
["J300300103","铅封螺钉","NW-M4*10(复合槽 不锈钢四孔穿线式南网专用)",550000]
["J300300102","铅封螺钉","NW-M4*31(复合槽 不锈钢四孔穿线式南网专用)",1100000]
["J300300347","铅封螺丝","M4*28(不锈钢，四孔穿线复合槽 南网专用)",400000]
["J300300329","铅封螺丝","M4*22，四孔穿线式，中碳钢镀三价铬环保彩锌，复合槽",40000]
["J300300328","铅封螺丝","M4*14，伞状，中碳钢镀三价铬环保彩锌，十字槽",40000]
["J300300327","铅封螺丝","M4*50，伞状，中碳钢镀三价铬环保彩锌，十字槽",40000]
["J300300299","铅封螺丝","国网铅封螺钉，M4×24，复合槽，中碳钢镀三价铬环保彩锌，20规范新标准，兼容穿线与嵌入",1200000]
["J210202084","铅封螺钉","M4×16，铁，镀彩锌，复合槽，四孔，LGG8.910.001",600000]
["J210202041","铅封螺钉","M4*8 铁镀彩锌，复合槽，四孔全螺纹（LGG8.910.001）",361000]
["J210202033","铅封螺钉","M4*36，铁，镀彩锌，复合槽，四孔（LGG8.910.001）",556000]
["J210202032","铅封螺钉","M4*20，铁，镀彩锌，复合槽，四孔（LGG8.910.001）",778000]
["J210202031","铅封螺钉","M4*25，铁，镀彩锌，复合槽，四孔（LGG8.910.001）",2060000]
["J210202029","铅封螺钉","M4*14，铁，镀彩锌，复合槽，四孔（LGG8.910.001）",2460000]
["J210202028","铅封螺钉","M4*30，铁，镀彩锌，复合槽，四孔（LGG8.910.001）",1005000]
["J210402012","压线螺钉","M5×10.5，碳钢，镀锌镍合金，镀层厚度>10μm，米字复合槽，柱头，符合RoHS，图号：LGG8.900.162K-01",1020000]
["J460300226","压线螺钉","M7×13.5，铁，镀环保彩锌，米字槽，LGG8.900.005",800000]
["J210106013","压线螺钉","M7×13.5，铜镀镍，米字槽，LGG8.900.005",481000]
["J210106012","压线螺钉","M6×14，中碳钢，镀三价铬环保彩锌，复合槽，盘头，LGG8.900.001",3128000]
["J210106008","压线螺丝","M6*14  铜镀镍 复合槽，盘头，LGG8.900.001",8400000]
["J210106006","压线螺钉","M4*12（铜镀镍，复合槽，盘头，LGG8.900.002）",24000]
["J210101004","压线螺钉","M6*14，铁，镀彩锌，复合槽，盘头（LGG8.900.001）",800000]
["J200300295","USB转DC充电线","USB转DC充电线，5V直通，DC3.5*1.35mm，电源线长度1m,图号：LGG8.510.014-B",195000]
["J200300277","磁阻采样线","SAN-5Y(针3.2)两端白壳线束L=46mm公差±3mm,UL2468 26AWG 5P红白排线",100000]
["J200300220","磁阻采样线","SAN-5Y(针2.2)黑壳/SAN-5Y(白壳)线束L=50mm,UL2468 26AWG 5P红白排线",700000]
["J200300121","8字电源线","欧标插头，1.5米",402000]
["J200300064","8字电源线","英标插头，1.5米",545000]
["J200200110","导线","L110-黑-1015两头剥线3mm",400000]
["J130100351","导热硅胶垫片","H150-A W6.5*T5.5*L6.5（mm）",160000]
["J130100202","高罩壳电池盒/圣帕","DDZY1122C-Z/-Z电池外置结构通用；20规范一体式结构；",1200000]
["J130100142","高罩壳电池座/圣帕","DDZY1122-M电池外置结构专用",1200000]
["J130100171","LED支撑柱","PC+GF10+FR，PANTONE 冷灰1U，图号：LGG8.154.001",140000]
["J130100131","吸铁板","29×16×t1.2，铁，镀彩锌，LGG8.160.002",140000]
["J130100117","硅胶按键","按键，硅橡胶，白色，12位，5号带盲点44.5*40.5*10mm，LGG8.730.005",697000]
["J130100114","硅胶按键","按键，硅橡胶，白色，12位，5号带盲点，45.4*41.4*21mm（LGG8.730.003）",1087000]
["J110100025","电流接线端片","31.2×31×2mm，黄铜H62，酸洗，带取压片，图号：LGG8.522.140K-01",50000]
["B070100075","气泡袋","LDPE，单面，气泡直径10mm，红色，防静电，窄边开口，尺寸：340*260mm，图号：LGG8.810.360K-01",25000]
["B070100073","EPE珍珠棉","EPE珍珠棉，尺寸要求：长220mm，宽160mm，厚10mm，图号：LGG8.835.380K-01",50000]
["B070100072","气泡袋","LDPE，单面，气泡直径10mm，白色，不防静电，窄边开口，尺寸220*160mm,图号：LGG8.810.540K-05",425000]
["B070100067","气泡袋","LDPE，单面，气泡直径10mm，红色，防静电，窄边开口，尺寸：280*210mm，图号：LGG8.810.160S-01",195000]
["B070100056","防静电气泡袋","LDPE，单面，气泡直径10mm，防静电，窄边开口，尺寸：240*180，图号：LGG8.810.140D-01",20000]
["B070100053","塑料袋","LDPE，220*150mm，t=0.04mm，LGG8.810.540K-03",402000]
["B070100048","PE自封袋","白边20丝（加厚），外形尺寸：16*24cm，窄边开口",1400000]
["B070100041","PE自封袋","PE自封袋，红边双层0.08mm厚，外形尺寸：90*130mm，窄边开口",80000]
["B070100034","PE袋","LDPE，400*550mm，t=0.04mm，窄边开口，图号：LGG8.810.611P-01",60000]
["B070100023","PE袋","LDPE，220*120mm，t=0.04mm，LGG8.810.002",140000]
["B070100028","塑料袋","LDPE，250*180mm，t=0.04mm，LGG8.810.004",20000]
["B070100024","塑料袋","260*360(LGG8.810.003)t=0.04mm",62000]
["B070100022","塑料袋","215*300（LGG8.810.001）LDPE t=0.04mm",430000]
["B060200137","220V 标示","标示为T型 短(图号NG0.364.21SNW1)",200000]
["B060200130","MC171贴纸","40*40（白色PET），带背胶，图号：LGG0.860.004",300000]
["B060200078","合格证","30*20（白色PET）图号：LGG0.860.001",1721000]
["B060100140","合格证","30*20（白色PET）图号：LGG0.860.017",100000]
["B060100139","合格证","30*17 (自动流水线使用)图号NG8.867.001(每卷10000只)",1260000]
["B060100115","合格证","水表，不干胶打印，图纸：NG8.868.HGZ1-B",800000]
["B060100014","干燥剂","3g",1740000]
["B050200003","木托盘","多层板，1160*880*120mm，动载1吨以上，图号：LGG8.820.362K-01",417]
["B050200002","木托盘","多层板，1250*850*120mm，动载1吨以上，图号:LGG8.820.160D-04",139]
["B050100235","木托盘","多层板，1040*900*120mm，动载1吨以上，图号：LGG8.820.540K-04",299]
["B050100233","木托盘","多层板，1060*980*120mm，动载1吨以上，图号：LGG8.820.380K-01",250]
["B050100148","木托盘","多层板，1080*840*120mm，动载1吨以上，图号:LGG8.820.160D-02",277]
["B050100128","木托盘","多层板，1130*950*120mm，动载1吨以上，图号：LGG8.820.100-01",132]
["B050100071","木托盘","多层板，1050*830*120mm，动载1吨以上，LGG8.820.016",494]
["B050100017","木托盘","多层板，1100*900*120mm，动载1吨以上，LGG8.820.004",328]
["B010100399","说明书","LGG540K，CIU说明书（SMS-041,IS1），材质：70g双胶纸",28000]
["B010100396","说明书","LGG540K，CIU说明书（SMS-038H,VR），材质：70g双胶纸，电表配套",24000]
["B010100388","说明书","LGG540K，CIU说明书（SMS-035H,IS2），材质：70g双胶纸，电表配套",250000]
["B010100368","说明书","SM-S003 DTZ1122/DTZY1122系列三相智能电能表(20版) ",127500]
["B010100366","说明书","LGG100，表说明书(SMS-031H)，材质：70g双胶纸，",10000]
["B010100362","说明书","LGG540K，CIU用户手册，材质：白色铜版纸，A4纸大小（297*210mm），三折页，彩色印刷",425000]
["B010100360","说明书","LGG100，表说明书（SMS-028H），材质：70g双胶纸，",100000]
["B010100346","说明书","SMS-D011",45834]
["B010100339","说明书","SM-S002",50000]
["B040500092","内包装下盖(第二版","1模5腔泡沫盒下盖， DN15/DN20：445*382*100mm",80000]
["B040500091","内包装上盖(第二版)","1模5腔泡沫盒上盖， DN15/DN20：445*382*72mm",160000]
["B040500087","内包装下盖","1模5腔泡沫盒下盖， DN15/DN20：445*382*100mm，图示：JS-LLW-12-175A",80000]

{"sheet":"议标清单","index":1,"n_rows":248,"n_cols":4,"rows_kept":248,"merged":[[211,0,217,0],[218,0,220,0],[221,0,223,0],[224,0,247,0]],"flags":["formulas_cached_only"]}
["物料编码","物料名称","规格","合计数量"]
["B030100060","纸浆托","39号(平均值：338g) 贵州单相 一托12只",291659]
["B030200014","纸浆托","565*365*60(图号NG8.839.19SNWYN1-3)上、下盖通用4只装",100000]
["B030200021","纸浆托","36号托  新疆三相 565*365*60 ",40000]
["B030200033","纸浆托","28号/国网三相 一托6 (模具调整)",143333]
["B040200054","包装箱","双瓦楞黄色牛皮纸A=B，开槽型（02型），415*350*295mm，尺寸图号：LGG8.832.020，版面图号：LGG8.832.020-PK01",3083]
["B040200121","包装箱","双瓦楞黄色牛皮纸A=B，开槽型（02型），375*315*285mm，24只装，图号：LGG8.832.100-01，版面图号：LGG8.832.100-01-PK02",4166]
["B040200131","包装箱","双瓦楞黄色牛皮纸A=B，开槽型（02型），375*255*285mm，24只装，图号：LGG8.832.100-02，版面图号：LGG8.832.100-02-PK01",416]
["B040200134","包装箱","双瓦楞黄色牛皮纸A=B，开槽型（02型），425*415*270mm，30只装，图号：LGG8.832.160D-03，版面图号：LGG8.832.160D-03-PK01",3333]
["B040200145","包装箱","双瓦楞黄色牛皮纸A=B，开槽型（02型），420*360*270mm，30只装，图号：LGG8.832.160D-02，空白版面",6666]
["B040200170","包装箱","双瓦楞黄色牛皮纸A=B，开槽型（02型），尺寸：530*490*365mm，尺寸图号：LGG8.832.380K-01，版面图号：LGG8.832.380K-01-PK01",3000]
["B040200172","包装箱","双瓦楞黄色牛皮纸A=B，开槽型（02型），520*445*315mm，尺寸图号：LGG8.832.540K-04，版面图号：LGG8.832.540K-04-PK01",4192]
["B040200178","包装箱","双瓦楞黄色牛皮纸A=B，开槽型（02型），560*365*235mm，尺寸图号：LGG8.832.140D-02，版面图号：LGG8.832.140D-02-PK01",1131]
["B040300105","包装箱","双瓦楞黄色牛皮纸A=B，开槽型（02型），365*300*285mm，6只装，尺寸图：LGG8.832.003，版面图：LGG8.832.003-PK11",2000]
["B040200188","包装箱","双瓦楞黄色牛皮纸A=B，开槽型（02型），尺寸：440*290*375mm,尺寸图号：LGG8.832.362K-01，版面图号：LGG8.832.362K-01-PK01",10000]
["B040300155","包装箱","双瓦楞黄色牛皮纸A=B，开槽型（02型），415*350*295mm，尺寸图号：LGG8.832.020，版面图号：LGG8.832.020-PK06",2083]
["B040300163","包装箱","双瓦楞黄色牛皮纸A=B，开槽型（02型），365*300*285mm，6只装，尺寸图：LGG8.832.003，空白版面",8333]
["B040300164","包装箱","双瓦楞黄色牛皮纸A=B，开槽型（02型），415*350*295mm，尺寸图号：LGG8.832.020，空白版面",5208]
["B040300190","包装箱","双瓦楞黄色牛皮纸A=B，开槽型（02型），390*360*285mm，6只装，尺寸图纸：LGG8.832.360K-06，版面图纸：LGG8.832.360K-06-PK02",166]
["B040200060","纸箱","580*380*180 单相 1/12 印子图NG8.839.314GZ20-2 尺寸图NG8.839.314GZ1",45833]
["B040200135","纸箱","580*380*180 单相 1/12 印子图NG8.839.314GZ20-2 尺寸图NG8.839.314GZ1 ",99999]
["B040300115","纸箱","575*374*240 贵州三相4只装（尺寸图号NG8.839.19SNWYN1-1 印字图号JS-DSN-07-001）",50000]
["B040300123","纸箱","575*374*240 重庆三相4只装（尺寸图号JS-DSG-08-002 印字图号JS-DSG-07-002）",20000]
["B040300156","纸箱","580*380*230山东三相 6只装 尺寸图：JS-DSG-08-008 印字图：JS-DSG-07-006",71666]
["B040200161","小纸盒","单瓦楞黄色牛皮纸B9B，折叠型（04型），205*115*90mm，LGG8.831.160D-01",20000]
["B040200169","小纸盒","单瓦楞黄色牛皮纸B9B，折叠型（04型），尺寸：235*170*102mm，图号：LGG8.831.380K-01",25000]
["B040200187","小纸盒","单瓦楞黄色牛皮纸B9B，折叠型（04型），尺寸：420*175*90mm，图号：LGG8.831.362K-01",60000]
["B040300056","小纸盒","单瓦楞黄色牛皮纸B9B，折叠型（04型），285*175*88mm，LGG8.831.003",62000]
["B050100069","隔板","双瓦楞黄色牛皮纸A=B，BC楞，尺寸400*330*7mm，图号：LGG8.833.008",31125]
["B050100083","隔板","单瓦楞黄色牛皮纸B9B，尺寸398*85*2mm，图号：LGG8.834.002-C",93375]
["B050100084","隔板","单瓦楞黄色牛皮纸B9B，尺寸336*85*2mm，图号：LGG8.834.002-D",225166]
["B050100125","隔板","双瓦楞黄色牛皮纸A=B，BC楞，尺寸360*125*7mm，图号：LGG8.834.100-01-C",8333]
["B050100126","隔板","双瓦楞黄色牛皮纸A=B，BC楞，尺寸300*125*7mm，图号：LGG8.834.100-01-D",41666]
["B050100127","隔板","双瓦楞黄色牛皮纸A=B，BC楞，尺寸350*300*7mm，图号：LGG8.833.100-01",8333]
["B050100142","隔板","加强型材料双瓦楞黄色牛皮纸A=B，BC楞，尺寸400*340*7mm，图号：LGG8.833.160D-02",20000]
["B050100144","隔板","双瓦楞黄色牛皮纸A=B，BC楞，尺寸400*75*7mm，图号：LGG8.834.160D-02-C",20000]
["B050100145","隔板","双瓦楞黄色牛皮纸A=B，BC楞，尺寸342*75*7mm，图号：LGG8.834.160D-02-D",80000]
["B050100173","隔板","双瓦楞黄色牛皮纸A=B，BC楞，尺寸350*240*7mm，图号：LGG8.833.100-02",833]
["B050100174","隔板","双瓦楞黄色牛皮纸A=B，BC楞，尺寸360*125*7mm，图号：LGG8.834.100-02-C",833]
["B050100175","隔板","双瓦楞黄色牛皮纸A=B，BC楞，尺寸240*125*7mm，图号：LGG8.834.100-02-D",4166]
["B050100183","隔板","双瓦楞黄色牛皮纸A=B，BC楞，尺寸410*75*7mm，图号：LGG8.834.160D-03-C",40000]
["B050100184","隔板","双瓦楞黄色牛皮纸A=B，BC楞，尺寸400*75*7mm，图号：LGG8.834.160D-03-D",10000]
["B050100185","隔板","加强型材料双瓦楞黄色牛皮纸A=B，BC楞，尺寸400*380*7mm，图号：LGG8.833.160D-03",10000]
["B050100230","隔板","加强型材料双瓦楞黄色牛皮纸A=B，BC楞，尺寸570*400*7mm，图号：LGG8.833.160D-04",155]
["B050100232","隔板","双瓦楞黄色牛皮纸A=B，BC楞，尺寸500*460*7mm，图号：LGG8.833.380K-01",3561]
["B050100236","隔板","双瓦楞黄色牛皮纸A=B，BC楞，尺寸500*90*7mm，图号：LGG8.834.540K-04-C",29250]
["B050100237","隔板","双瓦楞黄色牛皮纸A=B，BC楞，尺寸430*90*7mm，图号：LGG8.834.540K-04-D",97500]
["B050100239","隔板","双瓦楞黄色牛皮纸A=B，BC楞，尺寸500*420*7mm，图号：LGG8.833.540K-04",12186]
["B050100245","隔板","双瓦楞黄色牛皮纸A=B，BC楞，尺寸545*100*7mm，图号：LGG8.834.140D-01-C",6666]
["B050100246","隔板","双瓦楞黄色牛皮纸A=B，BC楞，尺寸350*100*7mm，图号：LGG8.834.140D-01-D",12222]
["J520603153","铜壳","DN20 铜质，浪花款，不带阀-用于无磁、磁阻采样",100000]
["J520200185","铜壳","DN15 铜质，浪花款，含阀杆密封圈-用于无磁、磁阻采样",400000]
["J520803085","铜壳","DN20 铜质，浪花款，含阀杆密封圈-用于无磁、磁阻采样",300000]
["J520200187","铜壳","DN25 铜质，浪花款，含阀杆密封圈-用于无磁、磁阻采样",0]
["J520200273","机芯（防冻专用叶轮）","DN15 与铜壳配套，5+1锁水机芯，中间磁阻采样（同步十升位，配宁光结构），表盘方向/字体方向（由上至下）与水流方向（由进水至出水）相同；表盘印字图：JS-LLW-23-012A",400000]
["J520200274","机芯（防冻专用叶轮）","DN20 与铜壳配套，5+1锁水机芯，中间磁阻采样（同步十升位，配宁光结构），表盘方向/字体方向（由上至下）与水流方向（由进水至出水）相同；表盘印字图：JS-LLW-23-012A",400000]
["J52200168","执行器","浪花款，线（红黑）长65±5mm，线端剥线吃锡2mm，配密封圈（密封圈材质：材质丁晴橡胶，规格外径17.5mm*线径2.4mm)",700000]
["Y030102001","压敏电阻","14K 681(420) 前后打弯 ",1632000]
["Y030103014","压敏电阻","20K 681(420)  L=3.5",120000]
["Y030103015","压敏电阻","MYG3 20K300(N)  L=3.5",190000]
["Y030103024","压敏电阻","MYL1-420/10(S)",550000]
["Y030103030","压敏电阻","MYG3-20K681(420) Φ19 L=3.5",80000]
["Y030103031","压敏电阻","MYG3-20K821(510) Φ19 L=3.5 ",2490000]
["Y030103041","压敏电阻","MYG3-20K510（WS）  （Φ19，H≤23.5mm，L=3.5）",40000]
["Y030103044","压敏电阻","MYL1-510/10（WST1) （最大冲击电流20kA，H≤29mm，L=3.5mm）",600000]
["Y030103028","压敏电阻","S20K510E2S26H23R9,9M3,5K77 爱普科斯",522000]
["Y030103045","压敏电阻","SIOV- S20K420E2S5H22M3,7K77 TDK",750000]
["Y030103048","压敏电阻","SIOV- S20K420E2S3M3,7K7 ",540000]
["Y080100019","法拉电容","1F/5.5V 扣式 (凯美) 温度范围：-40~+70 ℃”",400000]
["Y080100049","法拉电容","1.5F/5.5V 柱式 灌封（-40℃~85℃ ，脚中心距12mm）",1750000]
["Y080100056","法拉电容","0.22F 5.5V 柱式 灌封 （-40℃~85℃ ，脚中心距9mm）",710000]
["Y080100062","法拉电容","SDL（G）10F/2.7V  10*25 L=5.5mm",120020]
["Y080100075","法拉电容","SDL（G）10F/2.7V  10*25 L=11mm 卧式",250000]
["Y080100076","法拉电容","1.0F/5.5V扣式卧（凯美）温度范围-25℃~+70℃",376000]
["Y080100085","法拉电容","WEC 3R0 335 QG  3.3F 3V 插  8*20  L=3.5mm（-40℃~65℃) ",80000]
["Y080100089","法拉电容","2.5F/5.5V 柱式 灌封（-40℃~85℃ ，脚中心距12mm）插 L=8.5mm卧式 ",40000]
["Y080100096","法拉电容","HT-5R5-Z305VYA13(F39)(K08)(S03) 凯美",300000]
["Y080100098","法拉电容","1.5F/5.5V 柱式 灌封（-40℃~85℃ ，脚中心距12mm）插 L=8.6±0.5mm 卧式 ",800000]
["Y080100100","法拉电容","1.5F/5.5V 柱式 灌封（-40℃～85℃ ，脚中心距11.5±0.5mm）插 L=11±0.5mm 卧式 ",176000]
["Y100100078","集成电路","ATT7022FU 10*10贴 ",149000]
["Y100500024","集成电路","FM33LC046N 贴 ",500000]
["Y100500034","集成电路","FM33LC026N 贴",300000]
["Y100500038","集成电路","FM33LE026 (LQFP64) 贴",170000]
["Y100600029","集成电路","HT6015 贴",100000]
["Y100600038","集成电路","HT5017 贴 ",10000]
["Y100600041","集成电路","HT6019 贴 ",425000]
["Y100600042","集成电路","HT5023 贴 ",400000]
["Y100600046","集成电路","HT5027 贴 ",460000]
["Y100600047","集成电路","HT6035 贴",310000]
["Y100600053","集成电路","HT6033 贴",89000]
["Y100600058","集成电路","HT6025（K版）贴 ",550000]
["Y100600087","集成电路","HT6025(L) ",1200000]
["Y100600090","集成电路","HT5023E 贴 ",625000]
["Y101000051","集成电路","RN8209C 贴 编带",1750000]
["Y101000113","集成电路","RN8302B V32版 10*10 贴 ",400000]
["Y101000127","集成电路","RN8611 V22  贴",40000]
["Y101000131","集成电路","RN8318(14*14) V22 贴 ",400000]
["Y101100258","集成电路","DMHV-1400B 插 ",779000]
["Y101100262","集成电路","DM8233T 贴 ",947000]
["Y101100289","集成电路","DM8234T 贴 ",160000]
["Y101100293","集成电路","DM8234T 插 ",718000]
["Y101100301","集成电路","V9240 贴 ",120000]
["Y101100374","集成电路","DM7803SOPB#TRPBF SOP8 贴 ",630000]
["Y101100380","集成电路","DM8231H 插 ",910000]
["Y101100391","集成电路","DM7501 SOT23-5贴 ",140050]
["Y101100420","集成电路","V8530 贴 LQFP80",278000]
["Y101100445","集成电路","V9911 贴 ",100000]
["Y101100548","集成电路","6205H 贴 SOP8 ",150000]
["Y101100559","集成电路","DM6503 SOT23-5 贴 ",75000]
["Y101100561","集成电路","V9340 SOP-8 贴 ",75000]
["Y101100562","集成电路","V9400P LQFP100 贴 ",25000]
["Y101100578","集成电路","V9400 贴 ",200000]
["Y101100579","集成电路","DM8254T (DIP-7)插 ",340000]
["Y101100581","集成电路","6233K 插 ",25000]
["Y101100614","集成电路","V8500P 贴 ",60000]
["Y101100625","集成电路","6205H 贴 ",625000]
["Y101100627","集成电路","V8531 贴 LQFP-80Pin()",620000]
["Y101100648","集成电路","V8531(E2版本) 贴 LQFP-80Pin()",24000]
["Y101100661","集成电路","V9360D 贴 ",240000]
["Y101100662","集成电路","V8500(E版本) 贴 ",240000]
["Y100600052","计量芯片","HT7032 10*10贴",310000]
["Y101000109","计量芯片","RN8209D V4 贴 ",40000]
["Y101100536","温度传感器","7534SQNR QFN3x3-16 单相端子测温专用 贴 ",40000]
["Y180100019","锂电池","CR-P2 6.0V (双85,1000小时) ",710000]
["Y180200023","锂电池","ER14250 3.6V(宽引脚) ≥1200mAh ",1011050]
["Y180200029","锂电池","3.6V(无引脚) ≥1200mAh  ER14250 ",1750000]
["Y180200034","锂电池","F0179X-LF （带线）",1909000]
["Y180200055","锂电池","ER14250 F1557B 带电池盒 国网物联表盲样专用 ",40000]
["Y180400096","锂电池","CR17450 3.0V，线长225±10mm剥线3.5mm吃锡，防水(塑壳一体浇封)",300000]
["Y180400090","电池+SPC","ER26500容量电池+SPC1520， 3.6V，线长225±10mm剥线3.5mm吃锡,防水(使用宁光J521103026电池仓浇封)",500000]
["Y220100703","载波模块","XZ155D-NC （宁光海外定制版本程序）",20021]
["Y220100888","载波模块","XZ155E-NC ",100000]
["Y220100905","载波模块","XZ155DE-NC ",100144]
["Y220100979","载波模块","XZ1558XP-NC ",152000]
["Y220100980","载波模块","XZ1559BP-NC-2110001-DCC ",148020]
["Y220101057","宽带载波模块","XZ15575P-NC-2203001-STA",270000]
["Y220101060","宽带载波模块","XZ15575P-NC-2203001-CIU",270000]
["Y220101329","4G模块","EC200UEUAC-N05-SNNSA 贴",175000]
["Y220200097","模组","UC200AGLAA-N06-SNNSA  贴",425000]
["Y220200126","NB-IOT模块","BC28CNVAC-I01-CNASA",500000]
["Y220101402","蓝牙模块","HM-BT4531 ",850045]
["Y220101418","蓝牙模块","HZT810 V2.0 贴",40000]
["Y220200121","蓝牙模块","LSD4BT-E95ALSP001 ",300000]
["Y220101414","无线模块","LEC-RF1G1AC2 贴",45625]
["Y220100910","无线模块","LEC-RF1G0A 贴",1295000]
["Y270100085","继电器","WJ106-S-112DM ",710000]
["Y270100086","继电器","WJ106-S-112D ",30000]
["Y270100087","继电器","WJ106-S-112DB",300000]
["Y270100113","继电器","90A，180微欧，LGG5.565.013",20000]
["Y270100158","继电器","继电器，90A/250VAC，180uΩ，90A主体，1-4接，LGG5.565.031（版面规格印100A）",120000]
["Y270100176","继电器","继电器，90A/250VAC，250uΩ，90A主体，1-2接，LGG5.565.160K-01",600000]
["Y270100183","继电器","WJ106-S-112DB 带屏蔽罩",250000]
["Y270100189","继电器","100A/250VAC，180uΩ，100A主体，1-4接，LGG5.565.160D-01",200000]
["Y270100218","继电器","WJ31D 9VDC 90A 250VAC 250uΩ 硬连接 （无引线，南网21规范），对应2根铜柱J300300340",300000]
["Y270100225","继电器","100A/250VAC， 图号：LGG5.565.010-01",120000]
["Y270100226","继电器","100A/250VAC， 图号：LGG5.565.011-01",120000]
["Y270100273","继电器","HFE19 9VDC 60A 253VAC 260uΩ 硬连接（无引线，铜片1.2，正常隔磁罩，20规范，一体式方案 ），对应2根铜柱J300300322",1200000]
["Y270100302","继电器","国网20规范HFE45-NG-FDC-KDT-104N(七芯插头，绿绿红黄线长160mm，互感器从继电器底部出线) 焊接铜柱方案（配套铜柱编码J410400169，配套互感器编码：Y290200202） (Y)",300000]
["Y270300011","继电器","JZC-33F-012-ZS3 (555) ",62000]
["Y270300079","继电器","120A，锰铜阻值150μΩ，双硬连接，N相，图号:LGG5.565.380K-02",25000]
["Y270300102","继电器","60A，1-4接，锰铜阻值250微欧，带取压片，图号：LGG5.565.140K-03",50000]
["Y270300112","继电器","60A,1-2接，锰铜阻值250微欧，硬连接，带屏蔽罩，RoHS,图号LGG5.565.162K-01，",240000]
["Y270300113","继电器","60A,3-4接，带互感器（抗直流，5（60）A），硬连接，带屏蔽罩，RoHS,图号LGG5.565.162K-02，",240000]
["Y270100244","双联体继电器","2*90A，接线方式LNNL，主回路锰铜，阻值250微欧，副回路互感器，带后极取压线，图号：LGG5.565.160K-11",20000]
["Y270300068","双联体继电器","2x60A，主回路锰铜，阻值250微欧，不带后极取压线，图号：LGG5.565.160K-14",400000]
["Y270300098","双联体继电器","2*90A，接线方式LNNL，主回路锰铜，阻值250微欧，副回路抗直流互感器（5（80）A）（图号LGG5.600.180K-01，客供），不带后极取压线，图号：LGG5.565.180K-01-01",150000]
["Y270100296","三联体继电器","三联体继电器，120A，三路锰铜采样，阻值150μΩ，非对称式，不带后极线，图号：LGG5.565.380K-03",25000]
["Y270300059","三联体继电器","120A,带5(100)A互感器,非对称式,不带后极线,电压线插头防呆,图号：LGG5.565.360K-04-03",25000]
["Y270300064","三联体继电器","120A,带5(100)A互感器,非对称式,带长后极线,电压线插头防呆,图号：LGG5.565.360K-04-05",62000]
["Y270300120","三联体继电器","3*120A，带互感器（抗直流，5（80）A），非对称式，电压硬连接，RoHS,，图号：LGG5.565.362K-01",60000]
["Y270100301","继电器+电流互感器","HFE118 15-SDB-T-4-1 15VDC 100A 220VAC  100μΩ；HMCT238 5(100)A/2mA 10Ω 0.2级；对应1、2号铜柱J300300393，对应3、4号铜柱J300300394 ",40000]
["Y280100083","锰铜分流器","80A，180微欧，1-2接，图号：LGG5.575.100-03",110000]
["Y280100109","锰铜分流器","T2铜，阻值150微欧，带引线插头，图号：LGG5.575.360K-02",87000]
["Y280100137","锰铜分流器","阻值150μΩ，焊接导线，带SCN防呆插头，Rohs，图号LGG5.575.362K-01",60000]
["Y280100105","取样电阻","SGWFLQ-NW01 140μΩ 带两芯插头（线长180mm）、黑线长68mm、带焊接铜柱J410400157、最大载流量96A 南网专用 ",200000]
["Y280100116","取样电阻","SGWFLQ-AC04 170μΩ 带两芯插头（线长230mm）、黑线（带线鼻、套透明热缩套管、长35mm）、带焊接铜柱（铜柱编码J410400168）、最大载流量72A",400000]
["Y280100127","取样电阻","200μΩ （南网21规范送检得高分，全硬针，2.0mm厚，载流量96A)，对应2根铜柱J300300340",250000]
["Y290100087","电流互感器","(2合1三相三线用）ZY-F-20-120/160（GJD-KDT-178N）1.5（6）A/5mA 0.05级 20Ω 带八芯插头 带2mm屏蔽壳  初级铜片优化 焊接J410400199铜柱 康定通安 国网20规范",50000]
["Y290100089","电流互感器","(3合1三相四线用）ZY-F-20-120/140/160（GJD-KDT-178N）1.5（6）A/5mA 0.05级 20Ω 带八芯插头 初级铜片优化 焊接J410400199铜柱 康定通安 国网20规范",30000]
["Y290100097","电流互感器","(3合1三相四线表用)ZY-F-20-120/140/160（GJD-KDT-178N）1.5（6）A/5mA 0.05级 20Ω 带八芯插头 初级铜片优化  带J410400178焊接铜柱 康定通安 国网20规范送样专用",30000]
["Y290200084","电流互感器","5（80）A 2.5mA 0.2级/ 20Ω 外形：22.5*11mm 带引线 LGG5.600.004",20000]
["Y290200119","电流互感器","互感器，5（100）A，2mA，20Ω，0.1级，外形：22.7*10.8mm，脚间距16mm，带引线，LGG5.600.160D-04",320000]
["Y290200145","电流互感器","FDC-KDT-278C 5(60)A/2.5mA 0.2级 10Ω  康定通安（南网21规范、带焊针、插座、1.2Imax抗直流)内置表用，焊接铜柱J300300341",300000]
["Y290200165","电流互感器","（3合1）ZY-DJ-20-100/120/150(FDC-KDT-299)5(80)A/2mA 0.1级 10Ω（5A～96A防直流影响且相位差个体一致性控制在±20′，带八芯插头，二次引线线长A相100mm、B相120mm、C相150mm，带焊接铜柱J410400156 康定通安",200000]
["Y290200171","电流互感器","(3合1)ZY-DJ-20-90/110/140（FDC-KDT-104C) 5（60）A/2mA 0.1级 10Ω 加120A电流30min比差变差≤0.5%、相位变差≤8′（5A-72A防直流且相位差在345′-405′，带八芯插头）带J410400185焊接铜柱 康定通安",100000]
["Y290200191","电流互感器","FDC-KDT-313 5(80)A/2.5mA 0.2级 10Ω  康定通安（南网21规范、带焊针、插座、1.2Imax抗直流)外置表用，焊接铜柱J300300341",250000]
["Y290200193","电流互感器","5（80）A，2.5mA，20Ω，0.2级，外形：22.5*11mm，脚间距23mm，带取压片，带SCN-2Y插头，图号：LGG5.600.100-05",100000]
["Y290200201","电流互感器","5(80)A/2mA 0.2 10Ω  抗直流分量， 配双联体继电器LGG5.565.160K-14，申科",400000]
["Y290200202","电流互感器","国网20规范 (3合1加强磁通)FDC-KDT-104N 5(60)A/2mA 0.1级 10Ω， 5A-72A防直流影响且相位差控制在345′-405′，带八芯插头，次级线长为：A相140mm、B相165mm、C相215mm (配套继电器编码:Y270100288、Y270100302)",300000]
["Y290200221","电流互感器","5(80)A，2.5mA，10Ω，0.2级，外形：22.5*11mm，脚间距23mm，带SCN2.54插头，LGG5.600.160K-04，康定通安",600000]
["Y290200225","电流互感器","FDC-KDT-278 5(60)A/2.5mA 0.2级 10Ω 康定通安（带焊针、2.54mm中心距插座、1.2Imax抗直流，黑色壳体)，对应2根铜柱J300300302",1200000]
["Y290500040","电流互感器","5（80）A，2mA，10Ω，0.2级，抗直流，外形：28.5*17.8mm，带SCN防呆插头，图号：LGG5.600.180K-01，",150000]
["Y300100252","变压器","DB33K-220G1（满足双85要求）",550000]
["Y300100268","变压器","DB35K-220G3(新参数1，20版，满足双85要求;电气参数与WSD-DX-N一致)",1200000]
["Y300100233","高频变压器","JK-EE1348T ",20050]
["Y300100253","高频变压器","NG-EE16-01 ",947000]
["Y300100260","高频变压器","JK-EE1362T ",120000]
["Y300100269","高频变压器","NG-EF2068GS22A（参数改良，双85、1000小时） 插 ",630000]
["Y300100290","高频变压器","YZ2431-EE13 ",300010]
["Y300100315","高频变压器","JK-EF20166T ",88000]
["Y300100321","高频变压器","NG-EF1677NS2102（1、2脚对其它脚耐压4.2kV，6、7脚对其它脚耐压4.2kV,双85 1000小时）插",160000]
["Y300100329","高频变压器","YZ3273-EE13 ",645000]
["Y300100330","高频变压器","JK-EF20224T ",85000]
["Y300100342","高频变压器","LG-EPC17T2401 插 ",40000]
["Y300100346","高频变压器","JK-0425S 贴 ",75000]
["Y300300005","高频变压器","YZ3697-EF20 ",240000]
["J460400122","LGG631P三相普通表箱组件","表箱底(PC+ABS，PANTONE 冷灰 1U)+表箱盖(PC，透明)+透明视窗（PC，透明），带墙壁安装配件，外形尺寸：463*293*135mm",25000]
["J460400121","LGG611P单相普通表箱组件","表箱底(PC+ABS，PANTONE 冷灰 1U)+表箱盖(PC，透明)+透明视窗（PC，透明），带墙壁安装配件，外形尺寸：333*229*114mm",400000]
["J460400099","单相普通表箱组件","JG-D101A，表箱底(PC+ABS，PANTONE 冷灰 1U)+表箱盖(PC，透明)+墙壁安装配件，外形尺寸：333*229*105mm",50000]
["J460400098","单相一表位预付费表箱","表箱底（PC+ABS，PANTONE 冷灰 4U）+表箱盖（PC+ABS，PANTONE 冷灰 1U）+视窗（PC，透明）+断路器翻盖（PC，透明）+附件包（塑料膨胀管4+自攻螺钉4）",50000]
["J460400097","三相普通表箱组件","JG-S101A，表箱底(PC+ABS，PANTONE 冷灰 1U)+表箱盖(PC，透明)+墙壁安装配件，外形尺寸：463*293*125mm",25000]
["结构件/国家电网","A级单相费控智能电能表(远程-开关内置）","（远程-开关内置）0.25-0.5(60)A",1200000]
[null,"A级单相智能物联电能表（开关内置）","220V 0.25-0.5(100)A",40000]
[null,"B级三相费控智能电能表(远程-开关内置)","DTZY1122-M B级(远程-开关内置)\n3*220/380V 0.2-0.5(60)A",300000]
[null,"B级三相费控智能电能表(远程-开关外置)","DTZY1122-M B级(远程-开关外置)\n3*220/380V 0.2-0.5(60)A",100000]
[null,"C级三相费控智能电能表（远程-开关外置）","DTZY1122-M C级(远程-开关外置)\n3*220/380V 0.015-0.075(6)A",30000]
[null,"C级三相智能电能表(三相三线)","DSZ1122 C级\n3*100V 0.015-0.075(6)A",50000]
[null,"C级三相智能电能表（三相四线）","DTZ1122 C级\n3*57.7/100V 0.015-0.075(6)A",30000]
["结构件/南方电网","单相智能电能表","DDZ1122-M外置\n220V 0.25-0.5(80)A",250000]
[null,"单相智能电能表","DDZ1122-M内置\n220V 0.25-0.5(60)A",300000]
[null,"三相智能电能表（通信模块 -开关外置）","DTZ1122-Z B级\n3*220/380V 0.2-0.5(80)A",200000]
["结构件/流量表","NB-IOT智能水表\n铜壳，阀控","LGW-NHSQ40",400000]
[null,"NB-IOT智能水表\n铜壳，不带阀","LGW-NHSX30",100000]
[null,"IC卡智能水表\n蓝牙，铜壳，阀控","LSXY-01TLS",300000]
["结构件/海外电表","LGG160K-GH","LGG160K/LGG540K/LGGC80",400000]
[null,"LGG360K-GH","LGG360K/LGG540K/LGGC80",25000]
[null,"180K-NG","LGG180K/LGG540K/LGGC80",100000]
[null,"380K-NG","LGG360K/LGG540K/LGGC80",25000]
[null,"LGG140D-SA","LGG140D/LGG540K",20000]
[null,"LGG160D-ZA/MI","LGG160D/LGG540K",20000]
[null,"LGG140K-TZ","LGG140K/LGG540K",50000]
[null,"LGG180K-SE","LGG180K/LGG540K/LGGC80（同NG）",20000]
[null,"LGG180K-SL","LGG180K/LGG540K/LGGC80（同NG）",20000]
[null,"LGG180K-ML","LGG180K/LGG540K/LGGC80（同NG）",10000]
[null,"LGG160K-IS2","LGG160K/LGGC80(hplc)",300000]
[null,"LGG160D-IS2","LGG160D/LGG540K/LGGC80(hplc)",200000]
[null,"LGG360K-IS2","LGG360k/LGG540K/LGGC80(hplc)",50000]
[null,"LGG160K-KR1","LGG160K",300000]
[null,"LGG160K-IS1","LGG160K/LGGC80(东软G3模块)/LGG540",20000]
[null,"LGG360K-IS1","LGG360K/LGGC80(东软G3模块)/LGG540",8000]
[null,"LGG100-LS1","LGG100",100000]
[null,"LGG160D-GT1","LGG160D/LGG540K",100000]
[null,"LGG100-MN1","LGG100",10000]
[null,"LGG160K-MN1","LGG160K",5000]
[null,"LGG360K-MN1","LGG360K",1000]
[null,"LGG360T-MN1","LGG360T",1000]
[null,"LGG140D-KY","LGG140D/LGG540K",120000]
[null,"LGG360K-MZ","LGG360K/LGG540K",4000]

{"sheet":"远程议标清单","index":2,"n_rows":296,"n_cols":5,"rows_kept":296,"merged":[[113,0,113,4],[114,1,115,1],[116,1,152,1],[153,1,154,1],[155,1,236,1],[239,1,243,1],[244,1,250,1],[251,1,253,1],[254,1,259,1],[260,1,272,1],[273,1,281,1],[282,1,295,1]],"flags":["formulas_cached_only"]}
["存货编码","存货名称","规格型号","主计量单位","25年预算数量"]
["P0173010007","热缩套","φ50黄，10kV","米",350]
["P0173010008","热缩套","φ50绿，10kV","米",300]
["P0173010009","热缩套","φ50红，10kV","米",250]
["P0173010012","热缩套","φ60红，10kV","米",100]
["P0173010028","热缩套","φ80黄，10kV","米",200]
["P0173010029","热缩套","φ80绿，10kV","米",150]
["P0173010030","热缩套","φ80红，10kV","米",100]
["P0173010037","热缩套","φ30黄，10kV","米",200]
["P0173010038","热缩套","φ30绿，10kV","米",200]
["P0173010039","热缩套","φ30红，10kV","米",200]
["P0173010040","热缩套","φ40黄，10kV","米",350]
["P0173010041","热缩套","φ40绿，10kV","米",350]
["P0173010042","热缩套","φ40红，10kV","米",350]
["P0173020013","热缩套","φ25黄，1kV","米",1000]
["P0173020014","热缩套","φ25绿，1kV","米",1100]
["P0173020015","热缩套","φ25红，1kV","米",1200]
["P0173020020","热缩套","φ50黄，1kV","米",600]
["P0173020021","热缩套","φ50绿，1kV","米",600]
["P0173020022","热缩套","φ50红，1kV","米",600]
["P0173020023","热缩套","φ40黄，1kV","米",400]
["P0173020024","热缩套","φ40绿，1kV","米",700]
["P0173020025","热缩套","φ40红，1kV","米",700]
["P0173020026","热缩套","φ40蓝，1kV","米",300]
["P0173020027","热缩套","φ8黑，1kV","米",4000]
["P0173020028","热缩套","φ16红，1kV","米",1000]
["P0173020029","热缩套","φ16黄，1kV","米",1000]
["P0173020030","热缩套","φ16绿，1kV","米",1000]
["P0173020031","热缩套","φ35红，1kV","米",500]
["P0173020032","热缩套","φ35黄，1kV","米",500]
["P0173020033","热缩套","φ35绿，1kV","米",500]
["P0173020034","热缩套","φ80红，1kV","米",800]
["P0173020035","热缩套","φ80黄，1kV","米",800]
["P0173020036","热缩套","φ80绿，1kV","米",800]
["P0173020037","热缩套","φ100红，1kV","米",1000]
["P0173020038","热缩套","φ100黄，1kV","米",950]
["P0173020039","热缩套","φ100绿，1kV","米",900]
["P0173020046","热缩套","φ100蓝，1kV","米",200]
["P0173020048","热缩套","φ60黄，1kV","米",300]
["P0173020049","热缩套","φ60绿，1kV","米",400]
["P0173020050","热缩套","φ60红，1kV","米",300]
["P0173020051","热缩套","φ50蓝，1kV","米",200]
["P0173020052","热缩套","φ60蓝，1kV","米",300]
["P0173020053","热缩套","φ80蓝，1kV","米",400]
["P0173020063","热缩套","φ40黑，1kV","米",200]
["P0173020064","热缩套","φ35黑，1kV","米",200]
["P0172030005","管型预绝缘端头","E1008，易进线","个",60000]
["P0172030006","管型预绝缘端头","E1508，易进线","个",300000]
["P0172030007","管型预绝缘端头","E2508，易进线","个",200000]
["P0172030008","管型预绝缘端头","E4009","个",100000]
["P0172030009","管型预绝缘端头","E6012","个",26000]
["P0172030011","管型预绝缘端头","E16-12","个",7000]
["P0172030012","管型预绝缘端头","E25-16","个",6000]
["P0172030013","管型预绝缘端头","E35-16","个",4000]
["P0172030014","叉型预绝缘端头","SV1.25-3，易进线","个",210000]
["P0172030015","叉型预绝缘端头","SV2-4，易进线","个",60000]
["P0172030017","叉型预绝缘端头","SV3.5-6","个",4000]
["P0172030025","圆型预绝缘端头","RV2-6，易进线","个",60000]
["P0172030026","圆型预绝缘端头","RV2-8，易进线","个",40000]
["P0172030027","圆型预绝缘端头","RV3.5-6","个",3000]
["P0172030029","圆型预绝缘端头","RV5.5-8","个",4000]
["P0172030030","圆型裸端头","RNB8-6","个",4000]
["P0172030031","圆型裸端头","RNB8-8","个",26000]
["P0172030032","圆型裸端头","RNB14-8","个",12000]
["P0172030033","圆型裸端头","RNB14-10","个",3400]
["P0172030034","圆型裸端头","RNB22-8","个",5400]
["P0172030035","圆型裸端头","RNB22-10","个",1200]
["P0172030039","圆型裸端头","RNB70-12","个",200]
["P0172030047","叉型预绝缘端头","SV1.25-4，易进型","个",200000]
["P0172030048","圆形预绝缘端头","RV2-5，易进线","个",46000]
["P0172030049","插接端头","MPD1.25-156","个",30000]
["P0172030050","插接端座","FRD1-156","个",30000]
["P0172030052","圆型预绝缘端头","RV2-12，易进线","个",4000]
["P0172030053","圆型预绝缘端头","RV2-10，易进线","个",22000]
["P0172030054","圆型裸端头","RNB35-8","个",1200]
["P0172030055","圆型裸端头","RNB50-10","个",1000]
["P0172030056","圆型裸端头","RNB70-10","个",800]
["P0172030065","圆型裸端头","RNB50-8","个",2800]
["P0172030067","圆型裸端头","RNB80-12","个",600]
["P0172030068","管型预绝缘端头","E6010","个",2000]
["P0172030093","母全绝缘端头","FDFD2-250","个",2000]
["P0172030096","管型预绝缘端头","E1514，易进线","个",20000]
["P0172030103","圆型裸端头","RNB22-12","个",2000]
["P0172030104","圆型裸端头","RNB8-10","个",10000]
["P0172030105","圆型裸端头","RNB14-6","个",3000]
["P0172030112","管型预绝缘端头","E1512，易进线","个",2000]
["P0172030113","管型预绝缘端头","E1513，易进线","个",2000]
["P0172030114","管型预绝缘端头","E2510，易进线","个",2000]
["P0172030115","叉型预绝缘端头","150AM10，易进线","个",7000]
["P0108010001","电流端子","WURTKS/S","个",24000]
["P0108010002","电流端子挡板","D-URTKS/S","个",5000]
["P0108010003","电流连接条","FB10-URTK/SL","个",1800]
["P0108020002","普通端子挡板","D-UKS(4-10)G","个",2000]
["P0108020003","固定件","WE/UKS","个",22000]
["P0108020005","普通标记条","ZB5(1-10)LGS，白色","个",18000]
["P0108020007","普通标记条","ZB5 20 LGS，橙色","个",400]
["P0108020008","普通标记条","ZB5 30 LGS，橙色","个",200]
["P0108020009","普通标记条","ZB5 40 LGS，橙色","个",400]
["P0108020010","普通标记条","ZB5 50 LGS，橙色","个",200]
["P0108020011","普通标记条","ZB5 60 LGS，橙色","个",200]
["P0108020012","普通标记条","ZB5 70 LGS，橙色","个",400]
["P0108020013","普通标记条","ZB5 80 LGS，橙色","个",200]
["P0108020014","普通标记条","ZB5 90 LGS，橙色","个",200]
["P0108020015","普通标记条","ZB5 100 LGS，橙色","个",200]
["P0108020019","普通端子","SMWJ2-2.5","个",114000]
["P0108020020","挡板","SMWJ2-2.5G","个",9000]
["P0108020022","弹簧端子连接条","FBS3-5，3连","个",4000]
["P0108020023","弹簧端子连接条","FBS4-5，4连","个",6000]
["P0108020027","接地端子","SMWJ2-2.5-PE","个",4000]
["P0108040002","一次接线端子","WUKS10N","个",6000]
["P0108040003","一次接线端子","WUKS16N","个",1000]
["P0108090002","保险端子","SMWJ2-HESI","个",12000]
["P0108090003","挡板","SMWJ2-HESIG","个",8000]
["壳体因项目需求不同导致尺寸有差异只能按单台尺寸报价，25年壳体全年预计采购总额大约：800万元"]
["P0160040050","GGD低压柜","W600×H1800×D600","个",1]
["P0160040051",null,"W800×H1800×D800","个",1]
["P0160070064","动力柜柜体","W1000×H1800+100×D400","个",1]
["P0160070062",null,"W1000×H1800×D400","个",1]
["P0160070070",null,"W1000×H2000×D500","个",1]
["P0160070091",null,"W500×H1200+100×D400","个",1]
["P0160070089",null,"W500×H1800×D500","个",1]
["P0160070095",null,"W600×H1000+100×D400","个",1]
["P0160070050",null,"W600×H1250×D360","个",1]
["P0160070040",null,"W600×H1400×D400","个",1]
["P0160070065",null,"W600×H1600+100×D400","个",1]
["P0160070044",null,"W600×H1600×D400","个",1]
["P0160070047",null,"W600×H1600×D500","个",1]
["P0160070042",null,"W600×H1600×D600","个",1]
["P0160070072",null,"W600×H1700×D400","个",1]
["P0160070059",null,"W600×H1800×D400","个",1]
["P0160070078",null,"W600×H1800×D500","个",1]
["P0160070083",null,"W600×H1800×D600","个",1]
["P0160070093",null,"W700×H1200+100×D400","个",1]
["P0160070066",null,"W700×H1600+100×D400","个",1]
["P0160070075",null,"W700×H1600×D400","个",1]
["P0160070035",null,"W700×H1700×D400","个",1]
["P0160070067",null,"W700×H1800+100×D400","个",1]
["P0160070076",null,"W700×H1800×D400","个",1]
["P0160070079",null,"W700×H1800×D500","个",1]
["P0160070068",null,"W800×H1600+100×D400","个",1]
["P0160070077",null,"W800×H1600×D400","个",1]
["P0160070043",null,"W800×H1600×D600","个",1]
["P0160070087",null,"W800×H1700+200×D500","个",1]
["P0160070071",null,"W800×H1700×D400","个",1]
["P0160070069",null,"W800×H1800+100×D400","个",1]
["P0160070037",null,"W800×H1800×D400","个",1]
["P0160070080",null,"W800×H1800×D500","个",1]
["P0160070084",null,"W800×H1800×D800","个",1]
["P0160070039",null,"W800×H2000×D500","个",1]
["P0160070085",null,"W800×H2000×D600","个",1]
["P0160070092",null,"W900×H1200+100×D400","个",1]
["P0160070056",null,"W900×H1700×D500","个",1]
["P0160070057",null,"W900×H1800×D500","个",1]
["P0160080308","计量箱箱体","W700×H800×D180mm","个",1]
["P0160080190",null,"W900×H780×D180mm","个",1]
["P0160080184","配电箱箱体","W1000×H1300×D250mm","个",1]
["P0160080261",null,"W300×H400×D250mm","个",1]
["P0160080281",null,"W300×H450×D160mm","个",1]
["P0160080134",null,"W350×H400×D180mm","个",1]
["P0160080228",null,"W350×H450×D150mm","个",1]
["P0160080300",null,"W350×H450×D160mm","个",1]
["P0160080304",null,"W350×H500×D160mm","个",1]
["P0160080175",null,"W400×H300×D150mm","个",1]
["P0160080122",null,"W400×H300×D160mm","个",1]
["P0160080267",null,"W400×H300×D180mm","个",1]
["P0160080174",null,"W400×H500×D160mm","个",1]
["P0160080167",null,"W400×H500×D180mm","个",1]
["P0160080153",null,"W400×H500×D180mm","个",1]
["P0160080137",null,"W400×H500×D200mm","个",1]
["P0160080239",null,"W400×H500×D220mm","个",1]
["P0160080233",null,"W400×H500×D280mm","个",1]
["P0160080185",null,"W400×H600×D150mm","个",1]
["P0160080212",null,"W400×H600×D180mm","个",1]
["P0160080186",null,"W400×H800×D150mm","个",1]
["P0160080187",null,"W450×H1000×D180mm","个",1]
["P0160080188",null,"W450×H600×D160mm","个",1]
["P0160080136",null,"W450×H700×D200mm","个",1]
["P0160080166",null,"W450×H700×D220mm","个",1]
["P0160080123",null,"W500×H500×D160mm","个",1]
["P0160080271",null,"W500×H500×D180mm","个",1]
["P0160080162",null,"W500×H600×D180mm","个",1]
["P0160080303",null,"W500×H600×D200mm","个",1]
["P0160080217",null,"W500×H600×D220mm","个",1]
["P0160080249",null,"W500×H600×D250mm","个",1]
["P0160080225",null,"W500×H700×D120mm","个",1]
["P0160080168",null,"W500×H700×D180mm","个",1]
["P0160080259",null,"W500×H700×D200mm","个",1]
["P0160080238",null,"W500×H700×D220mm","个",1]
["P0160080310",null,"W500×H700×D250","个",1]
["P0160080296",null,"W500×H700×D250mm","个",1]
["P0160080189",null,"W500×H800×D160mm","个",1]
["P0160080222",null,"W500×H800×D250mm","个",1]
["P0160080241",null,"W500×H900×D250mm","个",1]
["P0160080221",null,"W550×H700×D180mm","个",1]
["P0160080282",null,"W550×H800×D200mm","个",1]
["P0160080250",null,"W600×H1000×D250mm","个",1]
["P0160080235",null,"W600×H1100×D250mm","个",1]
["P0160080128",null,"W600×H500×D150mm","个",1]
["P0160080145",null,"W600×H500×D180mm","个",1]
["P0160080151",null,"W600×H600×D180mm","个",1]
["P0160080283",null,"W600×H600×D200mm","个",1]
["P0160080215",null,"W600×H600×D250mm","个",1]
["P0160080227",null,"W600×H700×D180mm","个",1]
["P0160080278",null,"W600×H700×D200mm","个",1]
["P0160080158",null,"W600×H700×D220mm","个",1]
["P0160080279",null,"W600×H700×D250mm","个",1]
["P0160080224",null,"W600×H800×D120mm","个",1]
["P0160080160",null,"W600×H800×D180mm","个",1]
["P0160080135",null,"W600×H800×D200mm","个",1]
["P0160080214",null,"W600×H800×D220mm","个",1]
["P0160080124",null,"W600×H800×D250mm","个",1]
["P0160080273",null,"W600×H900×D250mm","个",1]
["P0160080216",null,"W700×H1000×D200mm","个",1]
["P0160080251",null,"W700×H1000×D250mm","个",1]
["P0160080120",null,"W700×H1100×D220mm","个",1]
["P0160080240",null,"W700×H1100×D350mm","个",1]
["P0160080140",null,"W700×H1200×D220mm","个",1]
["P0160080150",null,"W700×H600×D180mm","个",1]
["P0160080245",null,"W700×H700×D180mm","个",1]
["P0160080237",null,"W700×H800×D180mm","个",1]
["P0160080169",null,"W700×H800×D200mm","个",1]
["P0160080252",null,"W700×H800×D250mm","个",1]
["P0160080260",null,"W700×H900×D180mm","个",1]
["P0160080232",null,"W700×H900×D200mm","个",1]
["P0160080244",null,"W700×H900×D250mm","个",1]
["P0160080265",null,"W800×H1000×D200mm","个",1]
["P0160080149",null,"W800×H1000×D220mm","个",1]
["P0160080289",null,"W800×H1000×D250mm","个",1]
["P0160080159",null,"W800×H1000×D300mm","个",1]
["P0160080277",null,"W800×H1100×D200mm","个",1]
["P0160080275",null,"W800×H1100×D250mm","个",1]
["P0160080126",null,"W800×H800×D200mm","个",1]
["P0160080290",null,"W800×H800×D250mm","个",1]
["P0160080170",null,"W800×H900×D200mm","个",1]
["P0160080291",null,"W800×H900×D250mm","个",1]
["P0160080258",null,"W800×H900×D320mm","个",1]
["P0160080121",null,"W900×H1100×D200mm","个",1]
["P0160140002","GCK抽屉柜","W600×D1000×H2200","个",1]
["P0160140001","GCK固定柜","W1000×D1000×H2200","个",1]
["P0160030038","抽屉柜","1000×1000×2200","个",1]
["P0160030035",null,"1000×600×2200","个",1]
["P0160110019",null,"600×1000×2200","个",1]
["P0160030015",null,"800×1000×2200","个",1]
["P0160030024",null,"800×800×2200","个",1]
["P0160010016","高压柜","KYN28-12，W1000×D1500×H2300","个",1]
["P0160010028",null,"KYN28-12，W1000×D1800×H2300","个",1]
["P0160010029",null,"KYN28-12，W800×D1500×H2300","个",1]
["P0160010023",null,"KYN28-12，W800×D1600×H2320","个",1]
["P0160010024",null,"KYN28-12，W800×D1660×H2300","个",1]
["P0160010019",null,"KYN28-12，W800×D1700×H2320","个",1]
["P0160010030",null,"KYN28-12，W800×D1800×H2300","个",1]
["P0160020002","35kV柜","KYN61-40.5(II)，W1400×D2800×H2600","个",1]
["P0160020003",null,"KYN61-40.5(II)，W1400×D3000×H2600","个",1]
["P0160020004",null,"KYN61-40.5(II)，W1680×D2800×H2600","个",1]
["P0160030017","固定柜","1000×1000×2200","个",1]
["P0160030046",null,"1000×800×2200","个",1]
["P0160110015",null,"1200×1000×2200","个",1]
["P0160030019",null,"600×1000×2200","个",1]
["P0160110014",null,"800×1000×2200","个",1]
["P0160030023",null,"800×800×2200","个",1]
["P0160040024","GGD低压柜","W1000×H2000×D600","个",1]
["P0160040028",null,"W1000×H2200×D1000","个",1]
["P0160040040",null,"W1000×H2200×D600","个",1]
["P0160040042",null,"W1000×H2200×D800","个",1]
["P0160040043",null,"W1200×H2200×D800","个",1]
["P0160040030",null,"W600×H2000×D600","个",1]
["P0160040032",null,"W600×H2000×D800","个",1]
["P0160040022",null,"W600×H2200×D1000","个",1]
["P0160040053",null,"W600×H2200×D800","个",1]
["P0160040018",null,"W800×H2000×D600","个",1]
["P0160040031",null,"W800×H2000×D800","个",1]
["P0160040033",null,"W800×H2200×D600","个",1]
["P0160040015",null,"W800×H2200×D800","个",1]
["P0160050010","环网柜","HXGN15-12，W500×D1000×H2000","个",1]
["P0160050022",null,"HXGN15-12，W600×D1000×H2000","个",1]
["P0160050011",null,"HXGN15-12，W650×D1000×H2000","个",1]
["P0160050017",null,"HXGN15-12，W650×D1000×H2200","个",1]
["P0160050006",null,"HXGN15-12，W650×D900×H2000","个",1]
["P0160050013",null,"HXGN15-12，W700×D1000×H2000","个",1]
["P0160050023",null,"HXGN15-12，W800×D1000×H2000","个",1]
["P0160050009",null,"HXGN15-12，W800×D1000×H2200","个",1]
["P0160050016",null,"HXGN15-12，W900×D1000×H2000","个",1]
["P0160060013","箱式变电站","3300*1800*2540mm","台",1]
["P0160060024",null,"3300*2100*2540mm","台",1]
["P0160060016",null,"3400*2600*2540mm","台",1]
["P0160060026",null,"3600*2500*2540mm","台",1]
["P0160060023",null,"4000*2100*2540mm","台",1]
["P0160060019",null,"4200*2300*2540mm","台",1]
["P0160060027",null,"4200*2500*2560mm","台",1]
["P0160060022",null,"4300*2100*2540mm","台",1]
["P0160060020",null,"4300*2200*2540mm","台",1]
["P0160060025",null,"4500*2200*2540mm","台",1]
["P0160060021",null,"4900*2200*2540mm","台",1]
["P0160060015",null,"5100*2400*2540mm","台",1]
["P0160060017",null,"6000*2400*2540mm","台",1]
["P0160060014",null,"6100*2600*2540mm","台",1]